12.270.050 Development Standards


C. Protection of residential property.  Buildings in the MXD zone shall be separated from property lines when adjacent to Residential (R) zones as follows:

(1) for multi family residential: by amenities, interior accesses, surface parking, or open space in addition to a landscaped buffer of not less than ten feet (10’) in width and a solid screening fence or wall of not less than six feet (6’) in height; and

(2) for single family residential: by at least one line of single family residential homes with the MXD zoned parcel that are similarly situated to the adjacent Residential zone (in keeping with the development standards set forth in the R4 or R5 zones) or a landscaped buffer of not less than forty feet (40’) in width and a solid screening fence or wall of not less than six feet (6’) in height.

The development plan referenced in section 12.270.020(c) must comply with this section.






