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[bookmark: _in19xhbtkfni]6 - 1. Purpose and scope.
(1) The requirements of this chapter are intended to promote the orderly use of land and buildings by identifying minimum and maximum standards for accessory parking and loading facilities that will promote safe and convenient vehicular transportation andis chapter's requirements are intended to promote the orderly use of land and buildings by identifying minimum and maximum standards for accessory parking and loading facilities that will promote safe and convenient vehicular transportation and the movement of goods. These requirements are also intended tlso help lessen traffic congestion and promote a cleaner environment through reducing the number ofby reducing vehicle trips. Encouraging non- motorized transportation and relating parking requirements to the local land use/transportation system are is consistent with the objectives of this chapter.
(2) The off-street parking and loading provisions of this chapter shall apply to all buildings and structures erected and all uses of land established after the effective date of this chapter. Where a building permit has been issued prior to the effective date of this chapter and provided that construction is begun within six months of such effective date and diligently pursued to completion within 18 months of the effective date of this chapter, parking, and loading facilities in the amounts required for the issuance of said building permit may be provided in lieu of any different amounts required by this chapter. If such a building permit pertains to a stage of development only, any subsequent stage for which a building permit is required shall comply with the parking and loading requirements set forth in this chapter.
(3) When the intensity of any building, structure, or premises is increased through the addition of dwelling units, gross floor area, seating capacity, or other units of measurement specified herein for required parking or loading facilities, additional parking and loading facilities shall be provided in the amounts by which the requirements for the intensified use exceed those for the existing use. 
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6 - 2. Off-street parking required.
At the time any building or structure is erected, enlarged, increased in capacity, or any use is established, there shall be provided off-street parking spaces for automobilesoff-street parking spaces for automobiles shall be provided in accordance with the requirements of this chapter.
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6 - 3. Site plan requirements for a building permit.
Any application for a building permit shall include a site plan, drawn to scale and fully dimensioned, showing any off-street parking or loading facilities. 
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6 - 4. Access to individual parking spaces. 
Except for single-family and two-family dwellings, access to each parking space shall be from a private driveway and not from a public street. 
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6 - 5. Number of parking spaces.
(1) The minimum number of off-street parking spaces required shall be as follows: 

	Table 6.1 Parking Requirements

	Uses
	Requirement

	Athletic club, sports club/health spa
	4.37 spaces per 1,000 square feet of gross floor area

	Bank, located within a shopping center or store
	0.63 spaces per 1,000 square feet of gross floor area

	Bank
	4.23 spaces per 1,000 square feet of gross floor area

	Boarding house
	1 space for each room for rent, plus 2 spaces; 2 additional spaces if a portion of the building is used as a single dwelling unit

	Bowling alley
	2.36 spaces per lane

	Church
	One and one-quarter (13) spaces for each six feet of linear pew or four seats. However:
(i) Where a church building is designed or intended to be used by two congregations at the same time, two and one- quarter parking spaces shall be provided for each six feet of linear pew or four seats.
For buildings designed or intended to be used for conferences or other special meetings involving more than the regular congregations, the necessary parking shall be determined by the planning commission.

	Cleaning, servicing, testing or repair of materials or commodities
	1 space for each 3 employees

	Community center or recreational facility, for both commercial or private indoor
	
4 spaces per 1,000 square feet of gross floor space

	Daycare facility
	1 space for every 2 employees, plus 2 additional parking spaces, plus 1 loading space for every 8 clients

	Dwelling, multi-unit
	1.5 spaces for each residential dwelling unit

	Dwelling, single living unit
	2 spaces for each residential dwelling unit

	Residential facility for disabled and elderly persons, and assisted living facility
	
1 space for each 3 dwelling units

	Furniture/carpet/appliance store
	1.22 spaces per 1,000 square feet of gross floor area

	Gas station
	2 spaces for each employee, excluding spaces to serve the gas pumps

	Hospital
	1.79 spaces per bed

	Hotel/motel
	0.89 spaces per room, with restaurants figured separately

	Library, art gallery and museum
	2 spaces for each 1,000 square feet of gross floor area

	Light	industrial/manufacturing, wholesale stores, repair shops for household equipment and radio and television, and repair establishment
	
1.59 spaces per 1,000 square feet of gross floor area

	Machinery sales
	2.1 spaces per 1,000 square feet of gross floor area

	
Motor freight companies
	0.5 spaces per 1,000 square feet of gross floor area, plus 1 additional
space for each vehicle used in the conduct of the business at any time

	Motor vehicle sales
	2.1 spaces per 1,000 square feet of gross floor area

	Office, general
	2.79 spaces per 1,000 square feet of gross floor area

	Office, government
	3.84 spaces per 1,000 square feet of gross floor area

	Office, medical/dental clinic
	4.11 spaces per 1,000 square feet of gross floor area

	Paint/home	improvement/hardware store
	3.29 spaces per 1,000 square feet of gross floor area

	Private club and lodge
	1 space for each room for rent, plus 1 space for each 100 square feet of gross floor area, plus 1 space for each 4

	Production and manufacturing building
	1.59 spaces per 1,000 square feet of gross floor area

	Public utility and public services use
	1 space for each 3 employees, plus 5 spaces for public use

	Restaurant, bar, cafeteria and other eating and drinking places:
	

	Fast food restaurant with less than 21 seats
	0.5 spaces per seat

	Fast food restaurant with 21 or more seats
	14.14 spaces per 1,000 square feet of gross floor area

	Quality/family restaurant, cafeteria and bar/lounge
	15.89 spaces per 1,000 square feet of gross floor area

	Retail sales store, personal service establishment, shoe repair, barber and beauty shops, etc.
	
4.1 spaces per 1,000 square feet of gross floor area

	School, elementary, Jr high or boarding (except high)
	1 space for each 3 employees, plus 5 spaces

	School, high
	0.19 spaces per student

	Supermarket
	3.42 spaces per 1,000 square feet of gross floor area

	Theater and auditorium
	0.26 spaces per seat

	Warehousing or storage, not to include self-storage
	1 space per 1,000 square feet of gross floor area

	Other Uses:
For any other use not specifically mentioned or provided for in this Section, the zoning administrator shall determine the standards to be applied for parking, using as a guide the listed use which most closely resembles the use proposed or other recognized standard.


(2) The zoning administrator may authorize a reduction in the total number of required parking spaces for two or more uses jointly providing off- street parking when their respective hours of peak operation do not overlap. Shared parking shall be subject to the following conditions:
(a) The number of shared spaces for two or more distinguishable land uses shall be determined by the following procedurefollowing procedure shall determine the number of shared spaces for two or more distinguishable land uses:
(i) Multiply the minimum parking required for each individual use, as set forth in Table 6.1, by the appropriate percentage indicated in Table 6.2, Shared Parking Calculations, for each of the six designated time periods.  
(ii) Add the resulting sums for each of the six columns.
(iii) The minimum-parking requirement shall be the highest sum among the six columns resulting from the above calculations.
(iv) Select the time period with the highest total parking requirement and use that total as the shared parking requirement.
(b) Other uses. If one or all of the land uses proposing to make use of shared parking facilities do not conform to the general land use classifications in Table 6.2, Shared Parking Calculations, as determined by the zoning administrator, then the applicant shall submit sufficient data to indicate the principal operating hours of the uses. Based upon this information,
the zoning administrator shall determine the appropriate shared parking requirement, if any, for such uses.
(3) The maximum number of off-street parking spaced spaces for any building or use shall not exceed the amount determined as follows:
(a) Parking lots of more than 20 and less than 51 spaced: parking lots may not have more than 120% of the number of spaced identified in Table 6.1, not including accessible spaces, unless a minimum of 20 % of the parking area is landscaped in accordance with the standards of this chapter.
(b) Parking lots of 51 spaces or more: no more than 110% of the number of spaces requiredrequired spaces, as identified in Table 6.1 of this chapter, not including accessible spaces, is permitted. 
[bookmark: _rku5tiqb1lsg]6 - 6. Parking for the disabled.
(1) Any parking area to be used by the general public shall provide parking spaces designated and located to adequately accommodate the disabledccommodate the disabled adequately, and these shall be clearly marked as such. Parking spaces for the disabled shall be located in close proximity to the principal building. The designation of parking spaces for the disabled shall constitute consent by the property owner to the enforcement ofenforce the restricted use of such spaces to disabled motorists by the City. Parking spaces for the disabled shall conform to the standards of the Americans with Disabilities Act.
(2) The number of required parking spaces accessible to the disabled shall be as described in Tables 6.3 and 6.4. 


	Table 6.3 Minimum Required Accessible Parking Spaces

	
Total Parking Lot Spaces
	Required Minimum Number of Accessible Spaces

	1 to 25
	1

	26 to 50
	2

	51 to 75
	3

	76 to 100
	4

	101 to 150
	5

	151 to 200
	6

	201 to 300
	7

	301 to 400
	8

	401 to 500
	9

	501 to 1000
	2 percent of total

	1001 and over
	20, plus 1 for each 100
over 1000

	NOTE: See 6-10(3) for other use specific requirements





	Table 6.4 Van Parking Spaces Based on Required Parking Spaces

	
Total Accessible Parking Lot Spaces
	
Required Minimum Number of Accessible Spaces

	1 to 6
	1

	7 to 12
	2

	13 to 18
	3

	19 to 24
	4

	One additional van space for every six or fraction of six
required accessible parking spaces
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Adequate ingress and egress to and from all uses shall be provided as follows:
(1) All parcels and lots in all districts - Driveways shall comply with the following standards:
(a) In all Residential (R) and Residential Multi-family (RM) zoning districts, except for corner lots, all driveways shall access the road that the main building is facing, unless the driveway would result in an access on a collector or arterial road;
(b) corner lots may have a driveway access to no more than 2 two roads that it fronts unless prohibited below or by another law; and
(c) no access shall be made to a collector or arterial road except by local access roads unless the city engineer approves the access as being the only means of ingress and egress availablethe only means of ingress and egress.
(2) Residential Lots - For eEach residential lot less than one acre not more than two driveways shall have no more than two driveways, each of which shall not exceed 30 feet wide at the lot line immediately adjacent to the street. Lots one acre and larger but less than five acres shall have no more than three driveways, each of which shall not exceed 35 feet wide at the lot line immediately adjacent to the street, each of which shall be a maximum of 30 feet wide at the street lot line. Lots that are 5 acres or more may have an additional driveway for every 150 feet of street frontage, each of which shall not exceed 40 feet wide at the lot line immediately adjacent to the street.  Driveways shall not be closer than:
(a) 6 feet to a side or rear property line, and
(b) 40 Forty feet from any intersection on the side of the street where the driveway is located. The measurement is taken from the point of the intersection of the two converging front lot lines lying tangent to and in the same direction as the front lot lines, to the edge of the driveway.; and
(c) 20 Twenty feet to a driveway on the same parcel or lot.
(3) Other than Residential Lots - Access shall be provided to meet the following requirements:
(a) Not more than two driveways shall be used for each 100 feet or fraction thereof of frontage on any street.
(b) No two driveways shall be closer to each other than 12 feet, and no driveway shall be closer to a side property line than five feet. 
(c) Each driveway providing access to a single lot shall not be more than 35 feet wide, and each driveway providing access to two lots shall not be more than 50 feet wide per 100 feet of frontage, measured at right angles to the center line of the driveway, except as increased by permissible curb return radii. The entire flare of any return radius shall fall within the right-of-way.
(d) No driveway shall:
(i) be closer than 20 feet to the point of an intersection of two property lines;
(ii) be closer than 50 feet to the right of -of-way line of any road or street corner;
(iii) extend across any property line; , and
(iv) violate any conditions as shall be set forth in "Regulation for the control and protection of state highway rights of ways" by Utah Department of Transportation.et forth in the Utah Department of Transportation's "Regulation for the control and protection of state highway rights of ways."
(e) In all cases where there is an existing curb and gutter or sidewalk on the street, the applicant for a permit shall provide a parking strip, with a minimum width of ten feet, with a minimum width of ten feet along the entire frontage of the property, except for the permitted driveways. On the street side of the parking strip a concrete curb shall be constructed, the height and type is a six , a concrete curb shall be constructed, the height and type being a six-inch high back, unless another specification has been approved by the Department of Engineeringthe Department of Engineering has approved another specification.
(f) In planned unit developments, when required, and subdivisions that have a density greater than one acre lots, and there is no existing curb and gutter or sidewalk, the applicant shall install a parking strip, sidewalk, curb and gutter, unless this requirement is waived by the Department of EngineeringWhen required, in planned unit developments and subdivisions with a density greater than one-acre lot and no existing curb and gutter or sidewalk, the applicant shall install a parking strip, sidewalk, curb, and gutter unless the Department of Engineering waives this requirement. 
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[bookmark: _r5y3w2k7ncpj]6 - 8. Location of gasoline pumps.
  Gasoline pumps shall be set back not less thanat least 18 feet from any street line to which the pump island is vertical, and 12 feet from any street line to which the pump island is parallel, and not less than ten12 feet from any street line to which the pump island is parallel, and not less than 10 feet from any residential or agricultural district boundary line. If the pump island is set at an angle on the property, it shall be so located that the automobiles stopped for service will not extend over the property line. 
[bookmark: _huiyzkdr4l1a][bookmark: _r8sdvzh4icjf]6 - 9. Maintenance of parking lots.
Every parcel of land used as a public or private parking lot shall be developed and maintained in accordance with the following requirements:
(1) Each off-street parking lot shall be surfaced with an asphaltic or Portland cement or other binder pavement so as to provide a dustless surface. The parking area shall be so graded as to contain all surface water, by an onsphaltic, Portland cement, or other binder pavement to provide a dustless surface. site containment systemAn on-site containment system shall grade the parking area to contain all surface water. If such water is to be carried to adjacent streets, it shall be piped under sidewalks.
(2) The sides and rear of any non-residential off- street parking lot which faces or adjoins a residential district shall be screened from such district by a masonry wall or solid visual barrier fence not less than four nstreet parking lot that faces or adjoins a residential district shall be screened from such district by a masonry wall or solid visual barrier fence not less than four or more than six feet in height.
(3) Each parking lot shall be adequately landscaped and permanently maintained.
(4) Lighting used to illuminate any parking lot shall be arranged to reflect the light away from adjoining premises in any residential or commercial zoning district, and and from street traffic. 
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The dimensions for parking stalls and associated aisles are established in Table 6.2 with the following modifications and additions to those dimensions:
(1) Parking stalls located adjacent to walls or columns shall be one foot wider to accommodate door opening clearance and vehicle maneuvering ability.
(2) Parking angles between 0° and 45° and between 75° and 90° are not allowed. Requests for parking angles other than those shown on in Table
6.2 may be made to the planning commission.
(3) Handicapped parking spaces shall comply with the following standards:
(a) Regular handicapped parking stalls shall be 96" wide.
(bi) Van Van-accessible stalls shall be 132" wide but may be permitted to be 96" wide where the access aisle is 96" wide.
(c) All stalls shall have an access aisle with a width of no less than 60".
(d) The maximum slope in any direction shall be no greater than 1:50 (2%).
(e) Accessible routes must connect parking spaces to accessible entrances and be located on the shortest accessible route from parking to an accessible entrance. Where parking serves more than one accessible entrance, parking spaces shall be dispersed and located on the shortest accessible route to the accessible entrances.
(f) In parking facilities where the accessible route must cross vehicular traffic lanes, a marked crossing shall be made to enhance pedestrian safety, particularly for people using wheelchairs and other mobility aids.
(g) Parking spaces for vans, access aisles, and vehicle routes serving them shall provide a minimum height clearance of 98". 
(h) All parking spaces shall	be identified with the International Symbol of Accessibility. Signs identifying van spaces shall contain the designation “van accessible.” Signs shall be a minimum of 60" above the finished floor or ground measured to the bottom of the sign. Hospital outpatient facilities shall have ten percent of patient and visitor parking spaces set asideset aside ten percent of patient and visitor parking spaces for handicapped parking.
(i) Rehabilitation and outpatient physical therapy facilities specializing in treating conditions that affect mobility shall have 20 percent of patient and visitor parking spaces, physical therapy facilities, specializing in treating conditions that affect mobility shall reserve 20 percent of the patient and visitor parking spaces set aside for handicapped parking.
(j) Multi-family	residential	facilities shall provide the following:
(i) at least one parking space per dwelling unit is required to provide mobility features;
(ii) two percent with no less than one space for each residential dwelling that exceeds one parking space per unit.
(iii) parking spaces per Table 6.3, where spaces are provided for persons other than residents. 



	Table 6.5, Off-Street Parking Dimensions

	Parking
Angle
	Stall
Width
	Vehicle
Projection
	Aisle
Width
	Wall to Wall
Module Width
	Interlock
Reduction
	Overhang
Allowance

	0°
	22'00"
	9'00"
	9'05"
	27'05"
	0'00"
	2'00"

	45°
	9'00"
	16'10"
	12'06"
	46'04"
	2'03"
	2'00"

	50°
	9'00"
	17'05"
	13'03"
	48'01"
	2'00"
	2'00"

	55°
	9'00"
	17'11"
	13'11"
	49'09"
	1'10"
	2'01"

	60°
	9'00"
	18'03"
	14'07"
	51'01"
	1'07"
	2'02"

	65°
	9'00"
	18'06"
	15'06"
	52'06"
	1'04"
	2'03"

	70°
	9'00"
	18'07"
	16'04"
	53'06"
	1'01"
	2'04"

	75°
	9'00"
	18'06"
	17'10"
	54'10"
	0'10"
	2'05"

	90°
	9'00"
	17'06"
	22'07"
	57'07"
	0'00"
	2'06"
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