For Review
Chapter 1 – General Provisions & Introduction to Definitions
Section 1.6 – Buildable Area

Current wording
Buildable Area. The portion of a lot remaining after setbacks have been provided, except that land with an average grade exceeding fifteen percent (15%) shall not be considered buildable area unless it is approved by conditional use permit for construction, after study by a geologist, soils engineer, or sanitarian as required by the planning and zoning commission..

Proposed Wording
Buildable Area. The portion of a lot remaining after setbacks have been provided.

Reasons for proposed changes
1. The current definition, strays from the purpose of a definition with the wording “…shall not”.   
2. The remaining proposed changes are for improved grammatical flow.
3. Upon submission of a permit to build, the town appointed engineer would determine if the grade is or is not buildable as part of the process.
4. [bookmark: _GoBack]Other than the definition, the term “buildable area” does not appear anywhere in VULU.
