For Review
Chapter 20 – Commercial Zone
Section 20.15. – Architecture and Design
Sub Section .2

Current wording
20.15.2 – No unbroken exterior surface shall exceed 30 feet (30’) in length.  A surface is considered broken when interrupted by a protrusion or inlet of at least four feet (4’) extending the entire height of the wall.

Proposed Wording
20.15.2 – No unbroken exterior surface shall exceed fifty feet (50’) in length.  A surface is considered broken when interrupted by a protrusion or inlet of at least four feet (4’) extending the entire height of the wall.

Reasons for proposed changes
1. When looking at current allowable building size for the commercial zone, (2500 sq. ft. maximum); having a four foot protrusion every 30 feet, while restrictive in purpose, is counterproductive in actual construction feasibility the overall aesthetics that we are trying to achieve as a town according to our General Plan.  Expanding the distance to 50 feet provides the protections against large flat surfaces, while allowing for smaller buildings to have a clean, professional, aesthetically pleasing appearance.
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