For Review
Chapter 22 – Highway Resort Zone
Section 22.8 – Architecture and Design
Sub Section 4B

Current wording

22.8.4.B – No unbroken exterior surface shall exceed thirty feet (30’) in length.  A surface is considered broken when interrupted by a protrusion or inlet of at least four feet (4’) extending the entire height of the wall.

Proposed Wording

[bookmark: _GoBack]22.8.4.B – No unbroken exterior surface shall exceed fifty feet (50’) in length.  A surface is considered broken when interrupted by a protrusion or inlet of at least four feet (4’) extending the entire height of the wall.

Reasons for proposed changes
1. Although the Highway Resort Zone allows for larger building sizes than the Commercial Zone, expanding the distance between protrusions to 50 feet allows for smaller buildings to have a clean, professional, aesthetically pleasing appearance while still excluding the unwanted large flat surfaced buildings.
2. Having uniform architectural design between the two zones maintains the aesthetics across the town.
