Chapter 6
R-1 RESIDENTIAL ZONE

PROPOSED CHANGES AS OF 12/1/2020
Red = Addition, deletion, or change to existing specification
Green = Existing item reformatted or moved to a new location without change of specification



10-6-1: REGULATIONS:

The use, location, height and size of buildings and structures, the use of land and size of lots, yards, courts and other open spaces and the density of population are regulated as hereinafter set forth. (Ord. 2012-01, 7-10-2012)


10-6-2: INTENT:

The R-1 residential zone has been established for the purpose of providing a place where single family detached dwellings can be constructed, having attractively landscaped yards and a favorable environment for family life. Uses such as multiple-family dwellings, apartment houses and commercial and industrial uses are not permitted in this zone. (Ord. 2012-01, 7-10-2012)


10-6-3: PERMITTED USES:

A. The following buildings, structures and uses of land shall be permitted upon compliance with requirements set forth in this title:
Single-family dwellings of conventional construction and manufactured homes.
Foster care and family care homes.
Residential accessory uses and structures.
Churches, not including temporary revival tents or buildings.
Walls and hedges.
Household pets.
Machinery sheds used for storage of equipment used in connection with agricultural activities performed on the premises.
Public agency parks and playgrounds.
Public buildings and grounds not including storage yards and repair shops.
Public, private and parochial schools and grounds.
The growing of field crops and fruit.
The growing of fruit and gardens for household use.
Utility lines and buildings. (Ord. 2012-01, 7-10-2012)

B. The following uses are permitted when in compliance with the specified section of Title 10, Zoning Regulations: 
Accessory signs conforming to section 10-2-2 of this title.
Conditional uses as permitted in section 10-2-4 of this title.
Temporary uses subject to the provisions of section 10-2-6 of this title.
Keeping of chickens (please reference as allowed in section 10-2-8 of this title.
Fences in conformance with section 10-2-10.


10-6-4: AREA AND FRONTAGE REQUIREMENTS:

Area and frontage requirements shall be as follows:
	
Main Use
	
Minimum Lot Area
	Minimum Frontage (at setback line)

	Single family dwelling
	10,000 5,445 square feet
	80 60 feet

	Churches
	1 acre
	125 feet

	Other uses
	None
	None


(Ord. 2012-01, 7-10-2012)


10-6-5: LOCATION REQUIREMENTS:

Setback distances shall be determined by measuring from the property line to the foundation of the building.  All dwellings and other buildings and structures shall be set back according to the special conditions noted below:

A. Front Setback:
1. Main Buildings: All dwellings and other main buildings and structures shall be set back not less than twenty feet (20') from the front lot line back of curb.
a. If the narrowest distance from a resident's front property line and back of curb is greater than ten feet (10'), the owner's setback from property line may be reduced to ten feet (10').  Code exception only applicable to properties with curb to measure from. (Ord. 2014-4, 4-22-2014)
a. Where a curb is not present the setback shall be measured from the center of the city street as determined by the Public Works Department.
b. If a lot line is angled, a reduced setback requirement may be applied if all of the following conditions are met:
1. The narrowest distance from a resident’s front property line and back of curb is greater than ten feet (10’), and
2. The greatest distance is over twenty feet (20’), and
3. The setback conforms with surrounding homes.

1.	Main Setback:  All dwellings and other structures shall be set back according to the special conditions noted below:
a. Where the legal property line of the residential lot is located at the back of street curb or back of pavement and there is no curb, the front setback shall be twenty feet (20’) from the front lot line.
b. Where the legal property line of the residential lot is located within the street pavement or gravel area, the front setback shall be forty feet (40’) from the front lot line.
c. Where the legal property line of the residential lot is located more than ten feet (10’) from the street pavement or gravel area, the front setback shall be ten feet (10’) from the front lot line.  
d. Where the legal property line of the residential lot line is angular to the roadway and there is less than ten feet (10’) between the legal property line and the street pavement or gravel area, then the front setback shall be a minimum of twenty feet (20’) from the nearest point of the street pavement or gravel area.

	2.	Accessory Buildings: All accessory buildings shall be set back not less than twelve feet (12') to the rear of the closest rear wall line of the main building and not less than twelve feet (12') from any side wall of the main building. Accessory buildings which are located twelve feet (12') or closer to a main building shall be considered as part of the main building. Where no main building exists on a lot, a detached accessory building shall be set back not less than sixty feet (60') from the front lot line.

B. Side Setback; Interior Lots:
1. Main Buildings: All dwellings and other main buildings shall be set back at least eight feet (8') from the side lot line.
2. Accessory Buildings: All accessory buildings shall be set back at least five feet (5') from the lot line, except that no minimum side setback shall be required when all the following conditions are met:
a. The accessory building is located more than twelve feet (12') from any existing dwelling on the same or an adjacent lot;
b. The accessory building contains no openings on the side contiguous to the lot line;
c. No drainage from the roof will be discharged onto an adjacent lot.

C. Side Setback; Corner Lot:
1. Side Abutting A Street: All dwellings and other main and accessory buildings shall be set back at least twenty feet (20') from the side lot line which abuts on a street.
2. Interior Side: Same as required for interior lots.

D. Rear Setback; Interior Lots:
1. Main Buildings: All dwellings or other main buildings shall be set back at least thirty feet (30') from the rear lot line.
2. Accessory Building: Same as required under side setbacks; interior lots.

E. Rear Setback; Corner Lots:
1. Main Buildings: All dwellings and other main buildings shall be set back at least thirty feet (30') from the rear lot line, except that where a carport or garage is attached to the rear of the dwelling, the required rear setback for said carport or garage may be reduced to twenty feet (20') or more as measured from the rear lot line to the closest part of the building.
2. Accessory Building: All accessory buildings shall be set back at least five feet (5') from the rear lot line., except that no minimum rear setback shall be required when all the following conditions are met:
a. The accessory building is located more than twelve feet (12') from any existing dwelling on the same or an adjacent lot;
b. The accessory building contains no openings on the side contiguous to the lot line;
c. No drainage from the roof will be discharged onto an adjacent lot;
d. The accessory building will be set back at least fifty feet (50') from the side lot line abutting the street. (Ord. 2012-01, 7-10-2012)

F. 10-6-23: Exception To Front And Side Setback Requirements:
The setback from the street for any dwelling located between two (2) existing dwellings may be the same as the average for said two (2) existing dwellings, provided the existing dwellings are on the same side of the street and are located within one hundred fifty feet (150') of each other. (Ord. 2012-01, 7-10-2012)


10-6-6: HEIGHT OF BUILDINGS:

The maximum height of any building (measured from finished grade to the square of the building) shall be twenty feet (20') or two (2) stories, whichever is the higher. Where the ground or the square of the building is uneven in height, the average elevation thereof shall apply. Roofs about the square, chimneys, flagpoles, television antennas, church towers and similar structures not used for human occupancy are excluded in determining height. (Ord. 2012-01, 7-10-2012)  a dwelling building shall be measured from finished grade at the front of the dwelling to the highest wall plate.

A. The maximum height of a dwelling building shall be as noted below:
1. Level lot: Twenty-four feet (24’).
2. Uneven lot: Where the ground is uneven in height and the ground slopes downward from the front of the dwelling by more than ten feet (10’) to the back of the dwelling the maximum height shall be twenty feet (20’).


10-6-7: SIZE OF DWELLING:

The ground floor area of any single-family dwelling shall be at least nine hundred (900) square feet of living area exclusive of open porches, carports, garages and similar add ons. (Ord. 2012-01, 7-10-2012)


10-6-8: WIDTH OF BUILDINGS:

The total length or total width of any dwelling or church shall be at least twenty feet (20'), as measured from outside wall to outside wall, exclusive of any carport, garage, shed or similar add on. (Ord. 2012-01, 7-10-2012)


10-6-9: YARD SPACE FOR ONE MAIN BUILDING ONLY:

A. No required yard or other open space around an existing building, or which is hereafter provided around any building, that is needed to comply with the provisions of this title, shall be considered as providing a yard or open space for any other building; nor shall any yard or other required open space on an adjoining lot be considered as providing the yard or open space on the lot whereon a building is to be erected or established. (Ord. 2012-01, 7-10-2012)

B. No required yard or other open space around an existing main building, or which is hereafter provided around any building that is needed to comply with provisions of this title, shall be used for parking or storage of operable vehicles unless in compliance with 10-2-1.


10-6-10: EVERY DWELLING TO BE ON ZONING LOT:

Only one building which contains a dwelling shall be located and maintained on a "zoning lot" as defined in this title, except dwellings within a mobile home park, or other large scale development. (Ord. 2012-01, 7-10-2012)


10-6-11: SALE OR LEASE OF REQUIRED SPACE PROHIBITED:

No space needed to meet the width, yard, area, coverage, parking, or other requirements of this title for a lot or building may be sold or leased apart from such lot or building unless other space so complying is provided. (Ord. 2012-01, 7-10-2012)


10-6-12: YARDS TO BE UNOBSTRUCTED; EXCEPTIONS:

Every part of a required yard shall be open to the sky and unobstructed except:

A. Permitted accessory buildings, and 
B. Ordinary and customary projection of sills, belt courses, cornices and other ornamental features and unenclosed steps and unwalled stoops, porches and carports which may project up to three feet (3') into a required yard. No projection into a required court which is provided in connection with a court apartment shall be constructed except for customary sills, belt courses and cornices which may extend into a court not more than sixteen inches (16"). (Ord. 2012-01, 7-10-2012)


10-6-13: ACCESSORY BUILDINGS PROHIBITED AS LIVING QUARTERS:

Living and sleeping quarters in any building other than the main residential building are prohibited. (Ord. 2012-01, 7-10-2012)


10-6-14: STORAGE OF COMMERCIAL OR OVERSIZED VEHICLES
PROHIBITED:

The storage and/or continuous parking of trucks, buses, or a combination of vehicles exceeding thirty five feet (35') in length, or having a rated capacity of one ton or greater, and construction equipment such as bulldozers, graders, compressors, etc., shall not be permitted; provided, that construction equipment may be stored on a lot during construction of a building thereon for less than one year. Trucks and equipment parked in residential areas for more than three (3) days in any one month are not allowed. (Ord. 2012-01, 7-10-2012)
Storage of commercial or oversized vehicles shall comply with 10-2-3 of this title.


10-6-15: STORAGE OF JUNK, DEBRIS, OR UNLICENSED INOPERABLE VEHICLES PROHIBITED:

No yard or other open space surrounding an existing building, or which is hereafter provided around any building in any zone, shall be used for the storage of junk, debris or inoperable vehicles; and no land shall be used for such purposes, except as specifically provided by this title.  Storage of restorable vehicles may be permitted for a limited time, on a case by case basis, at the discretion of the zoning administrator. (Ord. 2012-01, 7-10-2012)


10-6-16: ADDITIONAL HEIGHT ALLOWED FOR PUBLIC BUILDINGS:

Public buildings and churches may be erected to any height, provided the building is set back from required building setback lines a distance of at least one foot (1') for each additional foot of building height above the maximum height otherwise permitted in the zone in which the building is located. (Ord. 2012-01, 7-10-2012)


10-6-17: MINIMUM HEIGHT OF DWELLINGS:

No dwelling shall be erected which has a ceiling height of less than seven feet six inches (7'6") eight feet (8’) or one story above grade, whichever is greater. (Ord. 2012-01, 7-10-2012)


10-6-18: SEWAGE DISPOSAL:

A. Sewer connections shall comply with section 8-4-2. 
B. Where domestic sewage disposal facilities are used which are not connected to a public sewer, approval of such facilities shall be obtained from the state health department before a building permit shall be issued therefor.  (Ord. 2012-01, 7-10-2012)


10-6-19: WATER CONNECTIONS:

A. Where municipal water is available all single family dwellings shall be connected in accordance with 8-4-2.
B. Where no municipal water is available, approval of such facilities shall be obtained from the state health department before a building permit or certificate of occupancy shall be issued therefore.


10-6-20: DRAINAGE:

A. The owners and users of ditches shall not divert more water into the ditch than its carrying capacity.  Runoff from new rooftops or lots shall not exceed the carrying capacity of the natural or previous drainage system. (Ord. 2012-01, 7-10-2012)
B. Drainage corridors shall be protected in accordance with 10-12-2.


10-6-21: CLEAR VIEW OF INTERSECTING STREETS:

No obstruction which will obscure the view of automobile drivers shall be placed on any corner lot within a triangular area formed by the street property lines and a line connecting them at points of forty five feet (45') forty feet (40’) from the intersection of the street lines. (Ord. 2012-01, 7-10-2012)


10-6-22: EFFECT OF STREET PLAN:

Wherever a front or side yard is required for a building that abuts on a proposed street which has not been constructed, but which has been designated by the planning commission as a future street, the depth of such front or side yard shall be measured from the planned street lines. (Ord. 2012-01, 7-10-2012)


10-6-23: MOTOR VEHICLE ACCESS:

Access to all lots and parcels of land having a frontage on a city street shall be controlled as follows:
A. Access shall be by not No lot shall have more than two (2) driveways from any one street.
B. Driveways shall not be closer to each other than twenty feet (20').
C. On corner lots, no driveways shall be closer than fifteen feet (15') twenty feet (20’) to the point of intersection of the front property line with the side property line which abuts upon a street.
D. Where there is no existing curb and gutter or sidewalk, a curb or fence may be required by the city. (Ord. 2012-01, 7-10-2012)


10-6-24: LANDSCAPING REQUIRED:

Front yards and side yards of all dwellings which front on city streets must be landscaped. (Ord. 2012-01, 7-10-2012)


10-6-25: POLLUTION PREVENTION:

Any use which emits or discharges gases, fumes, dust, glare, noise or other pollutants into the atmosphere in amounts which exceed the standards as prescribed by Utah state air conservation board or the board of health, and any use which emits or discharges liquids or solid material onto the soil or water in amounts which result in pollutants entering groundwater in amounts exceeding the standards prescribed by the Utah state water pollution control board or the board of health, shall be prohibited. (Ord. 2012-01, 7-10-2012)


10-6-26: SPECIAL PROVISIONS:

Special provisions shall apply in order to protect its essential characteristics.
A. All buildings used for human occupancy shall be furnished with a water supply in accordance with 10-6-19 of this title.
B. All buildings used for human occupancy shall be constructed in accordance with the adopted building, plumbing, electrical, fire prevention and similar codes.
C. All buildings and uses shall comply with all applicable supplementary development standards as set forth in this title. (Ord. 2012-01, 7-10-2012)

