G. Additional Construction Specifications:

1. No sign shall be erected, constructed, or maintained so as to obstruct any fire escape, required exit, window or door opening used as a means of egress.
2. No sign shall be attached in any form, shape, of manner which will interfere with any opening required for ventilation, except that signs may be erected in front of and may cover transom windows when not in violation of the provisions of the city building or fire prevention codes.
3. Signs shall be located in such way as to maintain horizontal and vertical clearance with all overhead electrical conductors in accordance with electrical code specifications, depending on voltages concerned.
4. Sign shall comply with the appropriate detailed provisions of the Building Code relating to design, structural members, and connections.
5. Signs shall also comply with the provisions of the National Electrical Code.
6. All signs must be inspected and approved by the building official upon completion.