Ordinance 2021-23
An Ordinance amending Ordinance 13.060.010 defining 
a temporary termination at property line

WHEREAS, the City Council of Hyde Park City, Cache County, Utah passed and adopted the Hyde Park City code on May 13, 2015; and
WHEREAS, The City Council of Hyde Park City determined there is a need to update, repeal, amend and/or modify certain provision contained in the referenced Municipal Code; and   
NOW, THEREFORE, that City Council of Hyde Park City, Utah hereby adopts, passes and published the following:
13.060.010 Minimum Improvement Requirements
C. Street Improvements. Layout of streets shall conform to sound engineering practices. Design of streets shall traverse slopes, where possible, and shall avoid, where practical, streets which run perpendicular to contour lines. Roads and other vehicles routes shall not cross property having a slope greater than twenty percent (20%) unless approved by the DRC and the Planning Commission, and it determines that appropriate engineering measures will be taken to minimize the impact of the cuts and fills, and that erosion control and slope stabilization will be performed. The environment and aesthetics of the area shall not be adversely affected. The layout and design of private roads and public right-of-way shall conform to the master plan and shall provide appropriate connections to adjacent properties and future roads.

Intersections of all streets shall be at 90º angles, unless topographic conditions exist and a different angle is determined appropriate by the DRC and the Planning and Zoning Commission. On all public streets, other than local residential streets, driveways may not be connected to the street. Subdivisions will be required to develop new streets perpendicular to public streets to minimize backing into traffic ways. Street signs shall be provided by the subdivider at all intersections as required by the City.

Total width of roads shall be the width shown on the master road plan, based on City cross-section standards. Other roads within the subdivision shall be sixty (60') feet. Sixty (60) foot wide roads will be permitted in cases where the road ultimately serves a street with a total of less than ten 10 homes. Cost of roads shall be borne by the subdivider.

Grades of road shall be a minimum of one-half of one percent (0.5%) and a maximum of twelve (12.0%) percent for local, collector, and arterial roads, on short, non sustained stretches of street, nor in excess of eight (8%) percent on sustained grades, unless otherwise modified or approved by the DRC, Fire Department and City engineer.

Asphalt surfacing shall be provided on all roads as indicated by the City’s current table of street cross-sections as determined by the City engineer.

Storm water inlets and catch basins shall be provided within the roadway improvements at points specified by the City engineer.

All curb corners shall have a radius of not less than twenty-five (25') feet. Where streets meet at acute angles, the radii shall be increased.

The arrangement of streets in a new subdivision shall make provision for the continuation of the existing streets in adjoining areas and shall provide access to unsubdivided adjoining areas insofar as such continuation or access shall be deemed necessary by the LUA and the Planning and Zoning Commission.
When a street has a temporary termination at the property line of an adjacent parcel, the developer has two options;
1. Obtain the right to create a fire dept. approved turnaround on the adjacent property.
2. Leave an empty lot on one side of the street to create the temporary turnaround until the street can be extended.
In either case there must be a pad to drive on that meets the fire dept. standards for a turnaround and it must be built to City street standards minus the asphalt or concrete cap.   
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New streets must connect with existing, improved public streets. An interim road may be required across adjacent properties unrelated to the development in order to connect for purposes of ingress and egress. All subdivisions must have a minimum of two roads for ingress and egress as accepted by the Land Use Authority and the Planning Commission.

Local streets shall approach the arterial or collector streets at an angle of not less than ninety (90) degrees for a minimum of forty (40) feet or the length of the flare on the intersection, unless conditions exist which prevent this. In no case shall the angle be less than eighty (80) degrees.

ADOPTED and PASSED by the Hyde Park City Council this 10th day of November 2021.

HYDE PARK CITY 					ATTEST



                                                              _______________________________
Charles Wheeler, Mayor			Donja Wright, City Recorder



