Request for Bids (RFB)
Lynndyl Town
Soliciting Body: Lynndyl Town
Project Title: Replacement Water Pump for High Flow Demand (Fire pump)
Project Funding: May be funded in part through HUD’s Community Development Block (CDBG) or other federal funding
Anticipated Project Start Date: October 2025
Bid Due Date: NOVEMBER 30, 2024, BY 4:00 P.M. MST


Overview
Lynndyl Town is seeking Competitive Sealed Bids (CSB) for procurement and installation of a water pump. The project may be funded in part through HUD’s Community Development Block Grant (CDBG) or other federal funding. The Town will select one (1) Contractor to provide equipment, materials, and labor for the project as outlined in this request. 
The project will consist of procuring a replacement water pump, all necessary components, installation, start-up, testing and training to operate and maintain the pump.

Scope of Work - Project requirements
Procurement and Construction Services
· Prepare unit pricing for materials and installation:
· High flow water pump Pentair Aurora Model 413SF Size 4X5X11A 800 GPM with 30HP 230 Volt 3 Phase electric motor, or equivalent,
· All additional necessary components
· Materials and installation of modified pad for pump (if required)
· Freight costs
· Installation of pump and all necessary components
· Start-up, testing and training to maintain and operate the pump
Quality of system components, quality of design, handicapped accessibility, inclusiveness, cost, appropriateness to location and target demographic must be taken into consideration in the design of the proposed system. Lynndyl requires contractors to provide equipment/materials that meets or exceeds all current federal standards, including ADA requirements. All installed parts must be of a commercial grade and quality. No residential grade equipment will be accepted.
The bid submitted needs to list the designed components being proposed for the replacement water pump and updates, as well as a time frame for completion once notified of award. Bidders should include structure and component model numbers, materials, color choices and recommendations, estimated lifetime of equipment including manufacturers’ warranty, and any other relevant descriptive information. Bidders are encouraged to take accessibility into account in their designs.
The water pump replacement and installation will be provided and managed by the Contractor. The Contractor must provide direct supervision from manufacturer or provide qualified and certified representative familiar with installation. All tools and equipment required shall be provided by the Contractor for this project.
A certified representative of the Town (Sunrise Engineering Inspector) is required to conduct a post construction/installation inspection of the water pump replacement and improvements and upgrades upon completion to insure proper installation. If not properly constructed/installed, modifications must be submitted in writing to the Town and remedied immediately. Co-inspection with a certified representative of the assembly and installation work will be conducted by a Town Representative. The Town will supply the punch list for final completion generated by this co-inspection. The Contractor shall submit to the manufacturer's certification of compliance and warranty following punch list completion.

Preferred Project Options
· All water pump installation elements must demonstrate the highest level of durability in materials and finishes selected in consideration of health and safety.
· "Green" construction practices and materials are highly desired.

Scope of Work and Terms and Conditions
The proposed Scope of Work has been included in this Request for Bids (RFB). Bidders should review the Scope of Work before submitting their responses to the Application requirements to ensure the Bidder’s capability to meet all project and funding requirements. Additional items that may be out for bid that are not included in this scope of work are NOT considered part of this project, but rather may be noted for information purposes.
The selected Bidder for this project is required to comply with the attached Terms and Conditions, attached Scope of work, and requirements of the CDBG funding source, including but are not limited to, compliance with HUD 4010 Federal Labor Standards, Section 3 of the Housing and Development Act of 1968, Build America, Buy America (BABA), and Department of Labor Davis-Bacon Wage Rates.

Post Award Document Requirements
The following documents may be required after notification of the bid award, prior to the execution of the agreement:
1. Worker’s Compensation Insurance
2. Comprehensive General Liability Insurance
3. Transportation Insurance
4. Business Licensing
5. Performance and Payment Bonds

Attachments
Attachment A: HUD 4010 Federal Labor Standards
Attachment B: Section 3 of the Housing and Development Act of 1968
Attachment C: Build America, Buy America (BABA)
Attachment D: Department of Labor Davis-Bacon Wage Rates

Contacts  
Lynndyl Town
Attn: Richard Pyne
98 East Center Street
Lynndyl, Utah 84640
Tel: (801) 376-9018
Email: rpyne@kinfolk.org


Submission Instructions
1. Two hard copies of bids must be submitted to Richard Pyne at Lynndyl Town Clerk's Office by 4:00 p.m. MST on November 30, 2024, at the address listed above.
2. Submitted bids must be addressed as follows:
Bid for Lynndyl Town Water Pump
Attn: Lynndyl Town Mayor Proctor
3. Two hard copies of bids shall be submitted in the following format:
a. Project Name
b. Supplier Name
c. Certification that Bidder will meet CDBG Guidelines, including previous experience of the Supplier and submission of required documentation from appendix A-D, as well as certification of understanding and compliance with Davis-Bacon Act
d. Designs showing all safety precautions necessary for this project as well as warranty and insurance capabilities
e. Project Cost of Proposal and Project Timeline
f. Any additional information related to scoring criteria
g. Minimum of two references of installations similar to this project. References shall include the name of the project, location, contact information including phone number, and general cost of installation.
h. Certified Check, Cashier’s Check, or Bid Bond

Additional Submission Information
1. Bidder must bear the cost of preparing and submitting a bid for this RFB. By submitting a bid for this project, Bidders acknowledge Lynndyl Town is exempt from any liability for costs incurred by unsuccessful bidders in the preparation of a competitive sealed bid.
2. Bids must include a bid price for each design presented in the proposal.
a. Bids must list the cost of equipment, materials, and labor separately.
b. Prices shall include freight on board (FOB), freight paid by the Bidder to the job site.
3. Bid amounts shall be guaranteed for not less than sixty (60) days after the Bids submittal deadline date.
4. Failure to comply with any part of the RFB may result in disqualification of the bid.
5. Late bids will not be accepted.
6. Bids that do not include all required documentation may not be considered complete and may be denied.
7. Lynndyl Town may request the correction of immaterial omissions during review. Bidder must respond within the time period provided in the request.
8. By submitting an application, the Bidder acknowledges and agrees that the requirements, Scope of Work, and the evaluation process outlined in this RFB are understood, fair, equitable, and are not unduly restrictive. Any exceptions to the content of this RFB must be addressed prior to the application deadline. The Bidder further acknowledges they have read the RFB, including Terms and Conditions and all attached or referenced documents.
9. Lynndyl Town is an Equal Employment Opportunity Entity. Qualified women, veterans, minority, and handicapped individuals are strongly encouraged to submit bids.

Bonding
[bookmark: _Hlk176446722][bookmark: _Hlk176446761]Each Bid must be accompanied by a Certified Check, Cashier’s Check, or Bid Bond payable to Lynndyl Town in an amount not less than ten percent (10%) of the total bid amount. The successful Supplier shall furnish approved Performance and Payment Bonds, each in the amount of one hundred percent (100%) of the bid amount. 

Addenda
Addenda shall be published within a reasonable time (at least 5 days prior to the application due date), to allow Bidders to consider the addenda when preparing applications. Minor addenda and urgent circumstances may require a shorter period of time. 

Evaluation and Award
1. Bids will be evaluated on a competitive basis, with award being made to the lowest qualified Bidder(s) whose CSB is determined to best meet the objectives of Lynndyl Town, taking into consideration all factors set forth in this RFB and outlined in the attached Evaluation Score Sheet.
2. Following the submission of all CSB submittals, a Selection Meeting, made up of the Council and the Mayor, will be held at 7:00 p.m. on December 4, 2024, in the Lynndyl Town Hall located at 98 East Center Street, Lynndyl Utah 84640. This meeting will be open to the public. All sealed bids shall be opened by the Mayor or designated representative in the above listed open public meeting, before one or more witnesses, at the time and place indicated in this bid packet.
3. This RFB is conducted in accordance with Utah State Procurement Code and Rule. Lynndyl Town will negotiate an agreement with the successful Bidder based on fair and reasonable compensation for the scope of work and services proposed.
4. Tied bids may be resolved using any reasonable criteria and at the sole discretion of Lynndyl Town
5. Lynndyl Town may reject any and all responses deemed unqualified, unsatisfactory or inappropriate at the sole discretion of Lynndyl Town.
6. Lynndyl Town reserves the right to reject any and all bids or withdraw this offer at any time.
7. Bidders must be available to answer clarifying questions during the grant review period.
8. Bidders must be available for presentations upon request.
9. Bids will be evaluated by a selection committee based on the following criteria:
a. Competence to perform the services as reflected by technical training and education, and direct experience in providing the services outlined herein. (20 points.
b. Project approach and familiarity with the town’s needs. (20 points
c. Past performance with installation culinary water pump services, including references and review of prior performance factors as control of costs, quality of work and the ability to meet deadlines. (30 points)
d. Organization and completeness of proposal (10 points
e. Cost proposal based on the Scope of Work (20 points)
f. Maximum Points: 100
10. Organizations previously receiving funding from Lynndyl Town should be in good standing to be considered under this RFB.
11. Submitted CSBs will be open to public inspection under the guidelines of the Government Records Access and Management Act (GRAMA). The entire application will be open unless bidder requests in writing that trade secrets/proprietary data be protected.  A GRAMA Claim of Business Confidentiality must be submitted to the prior to the submission deadline.

SUBMISSION CHECKLISTS
			
	Pre-Application Checklist

	
· 
	Unique Entity Identifier (UEI) number and Registration with SAM.gov (status must be active prior to receiving an executed agreement)

	· 
	Obtain or prepare project bond for CSB




	Application Checklist

	· 
	Proposed description, photos, and plans addressing RFB requirements

	· 
	Designs showing safety precautions necessary for the project

	
· 

	Compliance statement meeting CDBG Guidelines, including prior Bidder experience, as well as Compliance statement for applicable regulations, including Davis-Bacon and non-discrimination 

	· 
	Warranty and Insurance information and documentation 

	· 
	Project Timeline

	· 
	Cost Proposal

	· 
	Minimum of two references of comparable installations 

	· 
	Certified Check, Cashier’s Check, or Bid Bond for an amount not less than 10% of the total bid amount
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