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Request for Proposal: 
Extrication Tools, Fire Hose, Foam, PPE, and SCBA 







Uintah Fire Suppression Special Service District

         152 E 100 N Vernal, Utah 84078			                     Phone: (435) 781-6755
Fax: (435) 781-4962

Request Details

Uintah Fire Suppression SSD hereby makes notice of intent to solicit price quotation to provide for the purchase of extrication tools, fire hose, foam, and PPE. The specifications for extrication tools, fire hose, foam, PPE, and SCBA are listed below. The contract will last for 2 years and will begin on the day the request for proposal is awarded.

Price quotation must be clearly marked “Extrication, Fire Hose, Foam, PPE, and SCBA  Bid” and submitted by mail or delivered to the Uintah Fire Suppression SSD Office at 152 East 100 N Vernal UT 84078 and must be received no later than 3:00 pm on May 26, 2026. All bids received by this time will be opened but not awarded until the regularly scheduled District Meeting on May 27, 2026, at 5:15pm. The board meeting will be held at the Vernal City Office building located at 374 East Main Street in Vernal, Utah 84078. 

In comparing proposals, consideration will not be confined to price only. The successful bidder will be the one whose product is judged to best serve the interests of the Uintah Fire Suppression SSD when price, product, quality, and delivery are considered. Uintah Fire Suppression SSD reserves the right to reject any or all bids or any part thereof, and to waive any minor technicalities.

Uintah Fire Suppression SSD will not be held responsible for verbal statements of representation made by District personnel regarding the price quotation, not for any assumptions or conclusions reached by a prospective vendor because of such communication. No verbal communication will supersede these written specifications.

All questions pertaining to this RFP must be submitted by May 26, 2026 by 3:00pm. 

Please provide pricing and delivery information. 
The following equipment must meet or exceed the following specifications:

Extrication Tools
All tools will be battery operated. Meet current NFPA standards. Please list each manufacturer, the price, specifications, size and specs of each tool and any additional or extra add on costs. We need a quote on the following tools: Cutter, Spreader, Combination cutter/spreader, and rams. Also price any extra batteries and chargers. Bundle of tools and pricing can also be included.


Hose
All hose will be coupled and have NH threads. Structure hose will be double jacketed. Preferably made in the United States. Wildland hose will be single jacket 100% synthetic lightweight.  All hose must meet NFPA standards. Must specify pressures of hoses.

1.5” X 50’  			Structure Hose
1.75” X 50’ 			Structure Hose
2.5” X 50’ NH 			Structure Hose
3” X 50’ NH 				Structure Hose
5” X 25’, 50’, or 100 ’NH 		Structure Hose
1” X 50’ or 100’ NH or NPSH	Wildland Hose
1.5” X 50’ or 100’ NH or NPSH 	Wildland Hose 
¾” high pressure booster hose 
1” high pressure booster hose


Foam
Foam shall be supplied in 5-gallon pails, drums, or totes. Please provide pricing for each. List each brand name supplied and costs associated for each along with shipping. Foam must be PFAS free.

0.1 to 1%
1%
3%
6%
3 to 6% AFFF
3 to 6% AR-AFFF
MIL Spec for Airports
Encapsulated foam for lithium fires

If other foam is provided by vendor that’s not listed above, please list specifications and pricing.


PPE
Personal protective equipment will include structural and wildland gear. Please list each manufacturer/brand, the price, specifications, and any additional or extra add on costs.

Structure gear will include coat, pants, boots (leather or rubber) helmet, hood, and gloves.
Wildland gear will include nomex shirt and pants, boots, helmet, shroud, goggles, gloves, and packs.

Must list a specific quote for Globe turnouts including coat, pant, and boot(shadow).

SCBA
Submit pricing for MSA G1 airpacks. G1 4500 PSI with medium facepiece/nosecup 4 point adjustable cloth head harness, push to connect regulator, 60 min 4500 cylinder, 45 min 4500 cylinder, both with quick connect remote connection. Meet current NFPA standards. Include pack, bottles, masks, chargers, and any other additional or extra add on costs. Inlcude pricing for optional thermal imaging camera.



Proposals will not be accepted electronically.
Questions about the RFP can be directed to Jeremy Raymond, Director, by email to uintahfire@ubtanet.com or by phone at (435) 781-6756.
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