10.8.5 Schedule Of Minimum Area, Yard And Height Regulations
	District
	Dwelling Type
	Min. Lot Area
	Min. Lot Width (ft.)
	Min. Front Setback (ft.)
	Min. Side Setback (ft.)
	Min. Rear Setback (ft.)
	Min. Corner Lot Setback Front/Side (ft.)***
	Height Max.
	Driveway Setback (ft.)
	Lot Coverage By Bldg. (Max %)

	RR1-10
	One-family dwelling
	10 acres
	300
	50
	40
	40
	50
	35 ft.
	20
	10%

	R1-2
	One-family dwelling
	2 acres
	200
	50
	30
	30
	50
	35 ft.
	20
	25%

	*R1-2 PUD
	One-family dwelling
	2 acres
	200
	50
	15
	30
	50
	35 ft.
	20
	25%

	R1-1
	One-family dwelling
	1 acre
	150
	50
	30
	30
	50
	35 ft.
	20
	35%

	*R1-1 PUD
	One-family dwelling
	1 acre
	150
	50
	30
	30
	50
	35 ft.
	20
	35%

	R1-80
	One-family dwelling
	80,000 sq. ft.
	200
	50
	30
	30
	50
	35 ft.
	10
	25%

	R1-40
	One-family dwelling
	40,000 sq. ft.
	150
	50
	30
	30
	50
	35 ft.
	7.5
	25%

	R1-19
	One-family dwelling
	19,000 sq. ft.
	100
	30
	20/15
	30
	30
	35 ft.
	7.55
	25%

	**Mountain Villa Overlay Zone
	One-family dwelling
	19,000 sq. ft.
	60/65
	25
	Varies
10
	20
	30
	35 ft.
	5
	50%

	COM
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD

	Public
Facilities
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD

	Public Facilities
Mitigation- Zone
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD

	Public Facilities
Mitigation- Zone
No Trespassing
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD
	TBD



	*   Setback requirements for R1-1 PUD and R1-2 PUD are as shown, unless changed or modified in Article 10-10A governing planned unit development zones (PUDs)

	**   This zone comprises two lot sizes. One, an Estate Lot (larger lot), which is one-half acre 19,000 square feet or larger, and a Village Lot (smaller), which is less than one-half acre 19,000 square feet with a minimum size of ¼ acre (10,890 square feet). Setbacks for Estate lots are the same as for the R1-19 zoning; while setbacks for the Village Lot are as stated in section 10-10B-6.

	***   For all zones, corner lots shall have a side yard setback along the street equal to the front yard setback. Where the rear yard of a corner lot abuts the side yard of an adjacent lot, the rear yard setback of the corner lot shall be equal to the side yard setback of the adjacent lot if they are in the same zone. For accessory building setbacks, see City Code 10.11.2 and 10.11.3C(D).
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