17.52 OFF STREET PARKING						December 26, 2019

17.52.010 Off-Street Parking Required; Purpose
The purpose of this chapter is to set a minimum standard for off-street parking to ensure that ample parking for the generated demand of the use will be available.
Sufficient parking should be provided to assure maximum utilization of the facilities on site will not unduly impose on neighbors in the vicinity, or create an unsafe environment.
Off-street parking is required for residential, commercial, industrial and retail buildings and structures based on current use, size and capacity in accordance with the following requirements. 
At the time any building or structure is erected or enlarged or increased in capacity or any use is established, off-street parking spaces shall be provided for automobiles in accordance with the following requirements, or as otherwise required by conditional use permit. HISTORY
Adopted by Ord. 374-15 on 11/18/2015
17.52.020 Size
TThe dimensions of each off-street parking space, exclusive of access drives or aisles, shall be at least tennine (109) feet by twenty (20) feet for diagonal and ninety (90) degree spaces, and ten (10) feet by twenty-twofour (2224) feet for parallel spaces. However, in parking lots of not less than twenty (20) parking spaces, upon site plan approval by the planning commission, up to forty (40) percent of such spaces may be seven and one-half feet by fifteen (15) feet if marked and used for compact automobiles only. Drive aisle widths shall be a minimum of twenty-two (22) feet behind ninety (90) degree and parallel parking and sixteen (16) feet for angled parking.
HISTORY
Adopted by Ord. 374-15 on 11/18/2015
17.52.030 Access To Individual Parking Space
Except for single-family and two-family residential dwellings, direct access to each parking space shall be from a private driveway and not from a public street. All parking spaces shall have independent access not blocked by another parking space or other obstacle. 
HISTORY
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17.52.040 Number Of Parking Spaces Required
An adequate number of off-street parking spaces shall be provided for all uses as follows:
A. Business or professional offices: one parking space for each two hundred (200) square feet of floor area.
B. Churches with fixed seating: one parking space for each 3.5 fixed seats, or one parking space for each seven feet of linear pew, whichever is greater.
C. Churches without fixed seats, sports arenas, auditoriums, theaters, assembly halls, reception centers, meeting hallsrooms: one parking space for each three seats of maximum seating capacity.
D. 
E. Residential Dwellings: two parking spaces for each dwelling unit including garages and driveways.
F. Furniture and appliance stores: one parking space for each six hundred (600) square feet of floor area.
G. Hospitals: two parking spaces for each bed.
H. Hotels and motels: one space for each living or sleeping unit, plus parking space for all accessory uses as herein specified including employee parking.
I. Nursing homesResidential Health Care Facilities: four parking spaces, plus one parking space for each five beds, plus one parking space for each employee at the highest shift.
J. Restaurants, taverns, private clubs, and all other similar dining and/or drinking establishments: one parking space for each 3.5 seats or one parking space for each one hundred (100) square feet of floor area (excluding kitchen, storage, etc.), whichever is greater.
K. Retail stores (except as provided in subsection E of this section): one parking space for each one hundred (100) square feet of retail floor space.
L. Wholesale establishments, warehouses, manufacturing establishments and all industrial uses: as determined by conditional use permit or by planned unit development requirements if applicable, or by the planning commission zoning administrator, but in no case less than one space for each employee projected for the highest employment shift plus additional parking for vehicles used in conducting the business and customer parking.
M. Shopping center or other groups of uses not listed above: one parking space for each twoone hundred fifty (150200) square feet of total floor space, or as determined by conditional use permit.
N. Medical/Dental office: one parking space for each 200 square feet of gross floor area or five spaces per doctor, whichever is greater.
O. Fast Food: one parking space for each 75 square feet of floor area with a minimum of 5 spaces, plus 3 stacking spaces per drive-through lane.
P. Auto Dealer: one parking space for each 200 square feet of sales office area plus one space for every ten vehicles displayed, or five spaces, whichever is greater. Separate storage area for vehicles for sale or under repair shall be provided.
Q. Grocery Store: one parking space per every 200 square feet of floor area.
R. All other uses not listed above: as determined by conditional use permit zoning administrator based on the nearest comparable use standards, but in no case less than one space for each employee projected for the highest employment shift plus additional parking for vehicles used in conducting the business and customer parking.
S. 
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17.52.050 Access Requirements
Adequate ingress and egress to and from all uses shall be provided as follows:
1. Residential Lots. For eEach R-1-10, R-1-22, and A-1 residential lot, can have not more than two drive approaches which shall be a minimum of twelve (12) feet each and a maximum of thirty-two (32) feet wide at the property line, with a separation island of a minimum width of twelve (12) feet, and maximum combined drive approach width of thirty-two (32) feet on any single street frontage.  The drive approach flare entrance shall be no closer than four feet (4') to the abutting property line, or as approved by the City Engineer.  No driveway shall be closer than twenty (20) feet to the point of intersection of two property lines at any street corner as measured along the property lines.
2. Other Than Residential Lots. Access shall be provided to meet the following requirements:

1. Not more than two driveways shall be used for each one hundred (100) feet of frontage on any street;
2. No two of said driveways shall be closer to each other than twelve (12) feet, and no driveway shall be closer to a side property line than three feet;
3. Each driveway shall be not more than thirty-five (35) feet wide, measured at right angles to the center line of the driveway, except as increased by permissible curb return radii. The entire flare of any return radius shall fall within the right-of-way;
4. [bookmark: _Hlk23404417]No driveway shall be closer than twentyen (2010) feet to the point of intersection of two property lines at any street corner as measured along the property line, and no driveway shall extend across such extended property line; and
5. On a street where there are no curbs or gutters, all driveways shall be well marked and street frontage and pedestrian access protection provided the entire length of the frontage exclusive of the driveways as per approved plans.
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17.52.060 Maintenance Of Parking Lots
Every parcel of land used as a public or private parking lot shall be developed and maintained in accordance with the following requirements:
1. Surfacing. Each off-street parking lot shall be surfaced with gravel,an asphaltic or Portland cement or other binder pavement and permanently maintained so as to provide a dustless surface. The parking area shall be so graded as to dispose of all surface waterdesigned and maintained consistent with WBMC 13.30 Storm Water Management. If such water is to be carried to adjacent streets, it shall be piped under sidewalks.
2. Screening. The sides and rear of any off-street parking lot which adjoins an area which is to remain primarily residential shall be screened from such area by a masonry wall or solid visual barrier fence not less than four nor more than six feet in height.
3. Landscaping. Each parking lot shall provide along the entire frontage of the property a minimum depth of ten (10) feet of irrigated and permanently maintained landscaping. be adequately landscaped to comply with a plan approved by the planning commission and such landscaping shall be permanently maintained.
4. Lighting. Lighting used to illuminate any parking lot shall be directed downward be and arranged to reflect the light away from adjoining residential premises and from street traffic. 
5. All surfacing, screening, landscaping, lighting, and any other parking area elements shall be continually and properly maintained in good condition.
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17.52.070 Location Of Off-Street Parking
Off-street parking shall not be allowed in required front yard setbacks except by conditional use permit and in areas where the character of the street and general landscaping will not be adversely affected. Off-street parking in non-residential districts is allowed in the front setback provided that the parking area is set back a minimum ten (10) feet from the front property line, and the balance of the front yard setback along the entire frontage of the property is permanently landscaped.
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