60.3(a)

FLOOD DAMAGE PREVENTION ORDINANCE 20-04
ARTICLE I

STATUTORY AUTHORIZATION, FINDINGS OF FACT, PURPOSE AND METHODS

SECTION A. STATUTORY AUTHORIZATION

The Legislature of the State of Utah has in Utah Code Unannotated 10-3-701 delegated the responsibility

 to local governmental units to adopt regulations designed to promote the public health, safety, and 

general welfare of its citizenry. Therefore the City Council of Elk Ridge City does or has delegated the 
responsibility of local governmental units to adopt regulations designed to minimize flood losses. Therefore, 

does ordain as follows:

SECTION B. FINDINGS OF FACT

(1) The flood hazard areas of Elk Ridge City are subject to periodic

inundation, which results in loss of life and property, health and safety hazards, disruption of

commerce and governmental services, and extraordinary public expenditures for flood protection

and relief, all of which adversely affect the public health, safety and general welfare.

(2) These flood loses are created by the cumulative effect of obstructions in floodplains which cause an increase in flood heights and velocities, and by the occupancy of flood hazards areas by uses vulnerable to floods and hazardous to other lands because they are inadequately elevated, flood proofed or otherwise protected from flood damage.

SECTION C. STATEMENT OF PURPOSE

It is the purpose of this ordinance to promote the public health, safety and general welfare and to minimize public and private losses due to flood conditions in specific areas by provisions

designed to:

(1) Protect human life and health;

(2) Minimize expenditure of public money for costly flood control projects:

(3) Minimize the need for rescue and relief efforts associated with flooding and generally

            undertaken at the expense of the general public:

(4) Minimize prolonged business interruptions:

(5) Minimize damage to public facilities and utilities such as water and gas mains, electric,

            telephone and sewer lines, streets and bridges located in floodplains;

(6) Help maintain a stable tax base by providing for the sound use and development of flood-prone                          areas in such a manner as to minimize future flood blight areas; and

(7) Insure that potential buyers are notified that property is in a flood area.

SECTION D. METHODS OF REDUCING FLOOD LOSSES

In order to accomplish its purposes, this ordinance uses the following methods:

(1) Restrict or prohibit uses that are dangerous to health, safety or property in times of

flood, or cause excessive increases in flood heights or velocities:

(2) Require that uses vulnerable to floods, including facilities, which serve such uses, be protected against flood damage at the time of initial construction:

(3) Control the alteration of natural floodplains, stream channels, and natural protective barriers,        which are involved in the accommodation of flood waters;

(4) Control filling, grading, dredging and other development, which may increase flood damage;

(5) Prevent or regulate the construction of flood barriers which will unnaturally divert floodwaters or which may increase flood hazards to other lands.

ARTICLE 2

DEFINITIONS

Unless specifically defined below, words or phrases used in this ordinance shall be interpreted to

give them the meaning they have in common usage and to give this ordinance its most reasonable

application.

ALLUVIAL FAN FLOODING - means flooding occurring on the surface of an alluvial fan or

similar landform, which originates at the apex and is characterized by high-velocity flows: active

processes of erosion, sediment transport, and deposition; and unpredictable flow paths.

APEX - means a point on an alluvial fan or similar landform below which the flow path of the

major stream that formed the fan becomes unpredictable and alluvial fan flooding can occur.

AREA OF SHALLOW FLOODING - means a designated AO, AH, or VO zone on a

community's Flood Insurance Rate Map (FIRM) with a one percent chance or greater annual

chance of flooding to an average depth of one to three feet where a clearly defined channel does

not exist, where the path of flooding is unpredictable and where velocity flow may be evident.

Such flooding is characterized by ponding or sheet flow.

AREA OF SPECIAL FLOOD HAZARD - is the land in the floodplain within a community

subject to a one percent or greater chance of flooding in any given year. The area may be

designated as Zone A on the Flood Hazard Boundary Map (FHBM). After detailed ratemaking

has been completed in preparation for publication of the FIRM, Zone A usually is refined into

Zones A, AE, AH, AO, A1-99, VO, V1-30, VE or V.

BASE FLOOD - means the flood having a one percent chance of being equaled or exceeded in

any given year.

BASE FLOOD ELEVATION (BFE) is the water surface elevation of the 1-percent-annual-chance flood event.  It is the height in relation to mean sea level expected to be reached by the waters of the base flood at pertinent points in the floodplains of coastal and riverine areas. It is also the elevation shown on the FIRM and found in the accompanying Flood Insurance Study (FIS) for Zones A, AE, AH, A1-A30, AR, V1-V30, or VE that indicates the water surface elevation resulting from the flood that has a 1-percent chance of equaling or exceeding that level in any given year. 

BASEMENT - means any area of the building having its floor sub grade (below ground level) on

all sides.

CRITICAL FEATURE - means an integral and readily identifiable part of a flood protection

system, without which the flood protection provided by the entire system would be

compromised.

DEVELOPMENT - means any man-made change in improved and unimproved real estate,

including but not limited to buildings or other structures, mining, dredging, filling, grading,

paving, excavation or drilling operations or storage of equipment or materials.

ELEVATED BUILDING - means a non-basement building (i) built, in the case of a building in

Zones A1-30, AE, A, A99, AO, AH, B, C, X, and D, to have the top of the elevated floor, or in

the case of a building in Zones V1-30, VE, or V, to have the bottom of the lowest horizontal 

structure member of the elevated floor elevated above the ground level by means of pilings,

columns (posts and piers), or shear walls parallel to the flow of the water and (ii) adequately

anchored so as not to impair the structural integrity of the building during a flood of up to the

magnitude of the base flood. In the case of Zones A1-30, AE, A, A99, AO, AH, B, C, X, and D,

"elevated building" also includes a building elevated by means of fill or solid foundation

perimeter walls with openings sufficient to facilitate the unimpeded movement of flood waters.

In the case of Zones V1-30, VE, or V, "elevated building" also includes a building otherwise

meeting the definition of "elevated building," even though the lower area is enclosed by means of

breakaway walls if the breakaway walls met the standards of Section 60.3(e)(5) of the National

Flood Insurance Program regulations.

EXISTING CONSTRUCTION - means for the purposes of determining rates, structures for

which the "start of construction" commenced before the effective date of the FIRM or before

January 1, 1975, for FIRMs effective before that date. "Existing construction" may also be

referred to as "existing structures."

EXISTING MANUFACTURED HOME PARK OR SUBDIVISION - means a manufactured

home park or subdivision for which the construction of facilities for servicing the lots on which

the manufactured homes are to be affixed (including, at a minimum, the installation of utilities,

the construction of streets, and either final site grading or the pouring of concrete pads) is

completed before the effective date of the floodplain management regulations adopted by a

community.

EXPANSION TO AN EXISTING MANUFACTURED HOME PARK OR SUBDIVISION –means the preparation of additional sites by the construction of facilities for servicing the lots on

which the manufactured homes are to be affixed (including the installation of utilities, the

construction of streets, and either final site grading or the pouring of concrete pads).

FLOOD OR FLOODING - means a general and temporary condition of partial or complete

inundation of normally dry land areas from:

(1) the overflow of inland or tidal waters.

(2) the unusual and rapid accumulation or runoff of surface waters from any source.

FLOOD HAZARD BOUNDARY MAP (FHBM) - means an official map of a community,

issued by the Administrator, where the boundaries of the flood, mudslide (i.e., mudflow) related

erosion areas having special hazards have been designated as Zones A, M, and/or E.

FLOOD INSURANCE RATE MAP (FIRM) - means an official map of a community, on

which the Federal Emergency Management Agency has delineated both the areas of special flood

hazards and the risk premium zones applicable to the community.

FLOOD INSURANCE STUDY - is the official report provided by the Federal Emergency

Management Agency. The report contains flood profiles, water surface elevation of the base

flood, as well as the Flood Boundary-Floodway Map.

FLOODPLAIN OR FLOOD-PRONE AREA - means any land area susceptible to being

inundated by water from any source (see definition of flooding).

FLOODPLAIN MANAGEMENT - means the operation of an overall program of corrective

and preventive measures for reducing flood damage, including but not limited to emergency

preparedness plans, flood control works and floodplain management regulations.

FLOODPLAIN MANAGEMENT REGULATIONS - means zoning ordinances, subdivision

regulations, building codes, health regulations, special purpose ordinances (such as a floodplain

ordinance, grading ordinance and erosion control ordinance) and other applications of police

power. The term describes such state or local regulations, in any combination thereof, which

provide standards for the purpose of flood damage prevention and reduction.

FLOOD PROTECTION SYSTEM - means those physical structural works for which funds

have been authorized, appropriated, and expended and which have been constructed specifically

to modify flooding in order to reduce the extent of the areas within a community subject to a

"special flood hazard" and the extent of the depths of associated flooding. Such a system

typically includes hurricane tidal barriers, dams, reservoirs, levees or dikes. These specialized

flood modifying works are those constructed in conformance with sound engineering standards.

FLOOD PROOFING - means any combination of structural and non-structural additions,

changes, or adjustments to structures which reduce or eliminate flood damage to real estate or

improved real property, water and sanitary facilities, structures and their contents.

FLOODWAY (REGULATORY FLOODWAY) - means the channel of a river or other

watercourse and the adjacent land areas that must be reserved in order to discharge the base flood

without cumulatively increasing the water surface elevation more than a designated height.

FUNCTIONALLY DEPENDENT USE - means a use which cannot perform its intended

purpose unless it is located or carried out in close proximity to water. The term includes only

docking facilities, port facilities that are necessary for the loading and unloading of cargo or

passengers, and ship building and ship repair facilities, but does not include long-term storage or

related manufacturing facilities.

HIGHEST ADJACENT GRADE - means the highest natural elevation of the ground surface

prior to construction next to the proposed walls of a structure.

HISTORIC STRUCTURE - means any structure that is:

(a) Listed individually in the National Register of Historic Places (a listing maintained by

   the Department of Interior) or preliminarily determined by the Secretary of the Interior as

   meeting the requirements for individual listing on the National Register;

(b) Certified or preliminarily determined by the Secretary of the Interior as contributing to

the historical significance of a registered historic district or a district preliminarily determined   by the Secretary to qualify as a registered historic district;

(c) Individually listed on a state inventory of historic places in states with historic

     preservation programs which have been approved by the Secretary of Interior; or

(d) Individually listed on a local inventory or historic places in communities with historic

     preservation programs that have been certified either:

(1) By an approved state program as determined by the Secretary of the Interior or;

(2) Directly by the Secretary of the Interior in states without approved programs.

LEVEE - means a man-made structure, usually an earthen embankment, designed and

constructed in accordance with sound engineering practices to contain, control, or divert the flow

of water so as to provide protection from temporary flooding.

LEVEE SYSTEM - means a flood protection system which consists of a levee, or levees, and

associated structures, such as closure and drainage devices, which are constructed and operated

in accordance with sound engineering practices.

LOWEST FLOOR - means the lowest floor of the lowest enclosed area (including basement).

An unfinished or flood resistant enclosure, usable solely for parking or vehicles, building access

or storage in an area other than a basement area is not considered a building's lowest floor;

provided that such enclosure is not built so as to render the structure in violation of the

applicable non-elevation design requirement of Section 60.3 of the National Flood insurance

Program regulations.

MANUFACTURED HOME - means a structure transportable in one or more sections, which is

built on a permanent chassis and is designed for use with or without a permanent foundation

when connected to the required utilities. The term "manufactured home" does not include a

"recreational vehicle".

MANUFACTURED HOME PARK OR SUBDIVISION - means a parcel (or contiguous

parcels) of land divided into two or more manufactured home lots for rent or sale.

MEAN SEA LEVEL - means, for purposes of the National Flood Insurance Program, the

National Geodetic Vertical Datum (NGVD) of 1929 or other datum, to which base flood

elevations shown on a community's Flood Insurance Rate Map are referenced.

NEW CONSTRUCTION - means, for the purpose of determining insurance rates, structures for

which the "start of construction" commenced on or after the effective date of an initial FIRM or

after December 31, 1974, whichever is later, and includes any subsequent improvements to such

structures. For floodplain management purposes, "new construction" means structures for which

the "start of construction" commenced on or after the effective date of a floodplain management

regulation adopted by a community and includes any subsequent improvements to such

structures.

NEW MANUFACTURED HOME PARK OR SUBDIVISION - means a manufactured home

park or subdivision for which the construction of facilities for servicing the lots on which the

manufactured homes are to be affixed (including at a minimum, the installation of utilities, the

construction of streets, and either final site grading or the pouring of concrete pads) is completed

on or after the effective date of floodplain management regulations adopted by a community.

RECREATIONAL VEHICLE - means a vehicle which is (i) built on a single chassis; (ii) 400

square feet or less when measured at the largest horizontal projections; (iii) designed to be self-propelled or permanently towable by a light duty truck; and (iv) designed primarily not for use as

a permanent dwelling but as temporary living quarters for recreational, camping, travel, or

seasonal use.

START OF CONSTRUCTION - (for other than new construction or substantial improvements

under the Coastal Barrier Resources Act (Pub. L. 97-348)), includes substantial improvement and

means the date the building permit was issued, provided the actual start of construction, repair,

reconstruction, rehabilitation, addition, placement, or other improvement was within 180 days of

the permit date. The actual start means either the first placement of permanent construction of a

structure on a site, such as the pouring of slab or footings, the installation of piles, the

construction of columns, or any work beyond the stage of excavation; or the placement of a

manufactured home on a foundation. Permanent construction does not include land prep aeration,

such as clearing, grading and filling; nor does it include the installation of streets and/or

walkways; nor does it include excavation for basement, footings, piers or foundations or the

erection of temporary forms; nor does it include the installation on the property of accessory

buildings, such as garages or sheds not occupied as dwelling units or not part of the main

structure. For a substantial improvement, the actual start of construction means the first

alteration of any wall, ceiling, floor, or other structural part of a building, whether or not that

alteration affects the external dimensions of the building.

STRUCTURE - means a walled and roofed building, including a gas or liquid storage tank, that

is principally above ground, as well as a manufactured home.

SUBSTANTIAL DAMAGE - means damage of any origin sustained by a structure whereby the

cost of restoring the structure to its before damaged condition would equal or exceed 50 percent

of the market value of the structure before the damage occurred.

SUBSTANTIAL IMPROVEMENT - means any reconstruction, rehabilitation, addition, or

other improvement of a structure, the cost of which equals or exceeds 50 percent of the market

value of the structure before "start of construction" of the improvement. This includes structures

which have incurred "substantial damage", regardless of the actual repair work performed. The

term does not, however, include either: (1) Any project for improvement of a structure to correct

existing violations of state or local health, sanitary, or safety code specifications, which have been

identified by the local code enforcement official and which are the minimum necessary

conditions or (2) Any alteration of a "historic structure", provided that the alteration will not

preclude the structure's continued designation as a "historic structure." 

VARIANCE - is a grant of relief to a person from the requirement of this ordinance when

specific enforcement would result in unnecessary hardship. A variance, therefore, permits

construction or development in a manner otherwise prohibited by this ordinance. (For full

requirements see Section 60.6 of the National Flood Insurance Program regulations.)

VIOLATION - means the failure of a structure or other development to be fully compliant with

the community's floodplain management regulations. A structure or other development without

the elevation certificate, other certifications, or other evidence of compliance required in Section

60.3(b)(5), (c)(4), (c)(10), (d)(3), (e)(2), (e)(4), or (e)(5) is presumed to be in violation until such

time as that documentation is provided.

WATER SURFACE ELEVATION - means the height, in relation to the National Geodetic

Vertical Datum (NGVD) of 1929 (or other datum, where specified), of floods of various

magnitudes and frequencies in the floodplains of coastal or riverine areas.

ARTICLE 3

GENERAL PROVISIONS

SECTION A. LANDS TO WHICH THIS ORDINANCE APPLIES

The ordinance shall apply to all areas of special flood hazard within the jurisdiction of Elk Ridge City.

SECTION B. BASIS FOR ESTABLISHING THE AREAS OF SPECIAL FLOOD

HAZARD

Since areas of special flood hazard have not been identified, water surface elevations have not been provided, nor has sufficient data identifying the floodway been provided by the Federal Emergency Management Agency FEMA), the community shall obtain, review, and reasonably utilize data available from other Federal, State or other sources. 
 
The areas of special flood hazard identified by the Federal Emergency Management Agency in a scientific and engineering report entitled, The Flood Insurance Study for Utah County, dated June, 19, 2020 and accompanying Flood Insurance Rate Maps and Flood Boundary-Floodway Maps (FIRM and FBFM) and any revisions thereto are hereby adopted by reference and declared to be a part of this ordinance.

 
SECTION C. ESTABLISHMENT OF DEVELOPMENT PERMIT

A Development Permit shall be required to ensure conformance with the provisions of this

ordinance.

SECTION D. COMPLIANCE

No structure or land shall hereafter be located, altered, or have its use changed without full

compliance with the terms of this ordinance and other applicable regulations.

SECTION E. ABROGATION AND GREATER RESTRICTIONS

This ordinance is not intended to repeal, abrogate, or impair any existing easements, covenants,

or deed restrictions. However, where this ordinance and another ordinance, easement, covenant,

or deed restriction conflict or overlap, whichever imposes the more stringent restrictions shall

prevail.

SECTION F. INTERPRETATION

In the interpretation and application of this ordinance, all provisions shall be; (1) considered as

minimum requirements; (2) liberally construed in favor of the governing body; and (3) deemed

neither to limit nor repeal any other powers granted under State statutes.

SECTION G. WARNING AND DISCLAIMER OR LIABILITY

The degree of flood protection required by this ordinance is considered reasonable for regulatory

purposes and is based on scientific and engineering considerations. On rare occasions greater

floods can and will occur and flood heights may be increased by man-made or natural causes.

This ordinance does not imply that land outside the areas of special flood hazards or uses

permitted within such areas will be free from flooding or flood damages. This ordinance shall

not create liability on the part of the community or any official or employee thereof for any flood

damages that result from reliance on this ordinance or any administrative decision lawfully made

there under.

SECTION H. SEVERABILITY

If any section, provision, or portion of this ordinance is adjudged unconstitutional or invalid by a court, the remainder of the ordinance shall not be affected.

ARTICLE 4

ADMINISTRATION

SECTION A. DESIGNATION OF THE FLOODPLAIN ADMINISTRATOR

The City Recorder is hereby appointed the Floodplain Administrator to administer and implement the provisions of this ordinance and other appropriate sections of 44 CFR (National Flood Insurance Program Regulations) pertaining to floodplain management.

SECTION B. DUTIES & RESPONSIBILITIES OF THE FLOODPLAIN

ADMINISTRATOR
Duties and responsibilities of the Floodplain Administrator shall include, but not be limited to,

the following:

(1) Maintain and hold open for public inspection all records pertaining to the provisions of

      this ordinance.

(2) Review permit application to determine whether proposed construction or other

     development, including the placement of manufactured homes, will be reasonably safe from

  flooding.

(3) Review, approve or deny all applications for development permits required by adoption

of this ordinance.

(4) Review permits for proposed development to assure that all necessary permits have

been obtained from those Federal, State or local governmental agencies (including Section 404 of the Federal Water Pollution Control Act Amendments of 1972, 33 U.S.C. 1334) from which prior approval is required.

(5) Where interpretation is needed as to the exact location of the boundaries of the areas of

special flood hazards (for example, where there appears to be a conflict between a mapped

boundary and actual field conditions) the Floodplain Administrator shall make the necessary

interpretation.

SECTION C. PERMIT PROCEDURES

(1) Application for a Development Permit shall be presented to the Floodplain

  Administrator on forms furnished by him/her and may include, but not be limited to, plans in

  duplicate drawn to scale showing the location, dimensions, and elevation of proposed landscape alterations, existing and proposed structures, including the placement of manufactured homes,and the location of the foregoing in relation to areas of special flood hazard.

   Additionally, the following information is required:

a. Elevation (in relation to mean sea level), of the lowest floor (including basement)

    of all new and substantially improved structures;

b. Elevation in relation to mean sea level to which any nonresidential structure shall be

    flood proofed;

c. A certificate from a registered professional engineer or architect that the     nonresidential flood proofed structure shall meet the flood proofing criteria of Article 5, Section B(2); 

d. Description of the extent to which any watercourse or natural drainage will be altered or    relocated as a result of proposed development; and

e. Maintain a record of all such information in accordance with Article 4, Section B(1).

(2) Approval or denial of a Development Permit by the Floodplain Administrator shall be

based on all of the provisions of this ordinance and the following relevant factors:

a. The danger to life and property due to flooding or erosion damage;

b. The susceptibility of the proposed facility and its contents to flood damage and the

    effect of such damage on the individual owner;

c. The danger that materials may be swept onto other lands to the injury of others;

d. The compatibility of the proposed use with existing and anticipated development;

e. The safety of access to the property in times of flood for ordinary and emergency

 vehicles;

f. The costs of providing governmental services during and after flood conditions

 including maintenance and repair of streets and bridges, and public utilities and   facilities such as sewer, gas, electrical and water systems;

g. The expected heights, velocity, duration, rate of rise and sediment transport of the

 flood waters and the effects of wave action, if applicable, expected at the site;

h. The necessity to the facility of a waterfront location, where applicable;

i. The availability of alternative locations, not subject to flooding or erosion damage,

for the proposed use;

j. The relationship of the proposed use to the comprehensive plan for that area.

SECTION D. VARIANCE PROCEDURES

(1) The appeal Board as established by the community shall hear and render judgment on

   requests for variances from the requirements of this ordinance.

(2) The Appeal Board shall hear and render judgment on an appeal only when it is alleged

   there is an error in any requirement, decision, or determination made by the Floodplain

     Administrator in the enforcement or administration of this ordinance.

(3) Any person or persons aggrieved by the decision of the Appeal Board may appeal such

     decision in the courts of competent jurisdiction.

(4) The Floodplain Administrator shall maintain a record of all actions involving an appeal

   and shall report variances to the Federal Emergency Management Agency upon request.

(5) Variances may be issued for the reconstruction, rehabilitation or restoration of structures

   listed on the National Register of Historic Places or the State Inventory of Historic Places,

  without regard to the procedures set forth in the remainder of this ordinance.

(6) Variances may be issued for new construction and substantial improvements to be

erected on a lot of one-half acre or less in size contiguous to and surrounded by lots with     existing structures constructed below the base flood level, providing the relevant factors in Section C of this Article have been fully considered. As the lot size increases beyond the one-half acre, the technical justification required for issuing the variance increases.

(7) Upon consideration of the factors noted above and the intent of this ordinance, the

     Appeal Board may attach such conditions to the granting of variances as it deems necessary to

     further the purpose and objectives of this ordinance (Article 1, Section C).

(8) Variances shall not be issued within any designated floodway if any increase in flood

   levels during the base flood discharge would result.

(9) Variances may be issued for the repair or rehabilitation of historic structures upon a

determination that the proposed repair or rehabilitation will not preclude the structure's   continued designation as a historic structure and the variance is the minimum necessary to preserve the historic character and design of the structure.

(10) Prerequisites for granting variances:

a. Variances shall only be issued upon a determination that the variance is the

 minimum necessary, considering the flood hazard, to afford relief.

b. Variances shall only be issued upon, (i) showing a good and sufficient cause; (ii) a 

determination that failure to grant the variance would result in exceptional hardship to the applicant, and (iii) a determination that the granting of a variance will not result in increased flood heights, additional threats to public safety, extraordinary public expense, create nuisances, cause fraud on or victimization of the public, or conflict with existing local laws or ordinances.

c. Any application to whom a variance is granted shall be given written notice that

the structure will be permitted to be built with the lowest floor elevation below the base    flood elevation, and that the cost of flood insurance will be commensurate with the increased risk resulting from the reduced lowest floor elevation.

(11) Variances may be issued by a community for new construction and substantial

improvements and for other development necessary for the conduct of a functionally    dependent use provided that (i) the criteria outlined in Article 4, Section D(1)-(9) are met, and (ii) the structure or other development is protected by methods that minimize flood damages during the base flood and create no additional threats to public safety.

ARTICLE 5

PROVISIONS FOR FLOOD HAZARD REDUCTION

SECTION A. GENERAL STANDARDS

In all areas of special flood hazards the following provisions are required for all new construction

and substantial improvements.

(1) All new construction or substantial improvements shall be designed (or modified) and

adequately anchored to prevent flotation, collapse or lateral movement of the structure resulting from hydrodynamic and hydrostatic loads, including the effects of buoyancy;

(2) All new construction or substantial improvements shall be constructed by methods and

   practices that minimize flood damage;

(3) All new construction or substantial improvements shall be constructed with materials

   resistant to flood damage;

(4) All new construction or substantial improvements shall be constructed with electrical,

heating, ventilation, plumbing, and air conditioning equipment and other service facilities that are designed and/or located so as to prevent water from entering or accumulating within the

   components during conditions of flooding.

(5) All new and replacement water supply systems shall be designed to minimize or

  eliminate infiltration of flood waters into the system;

(6) New and replacement sanitary sewage systems shall be designed to minimize or

eliminate infiltration of flood waters into the system and discharge from the systems into flood

   waters; and,

(7) On-site waste disposal systems shall be located to avoid impairment to them or

   contamination from them during flooding.

SECTION B. STANDARDS FOR SUBDIVISION PROPOSALS

(1) All subdivision proposals including the placement of manufactured home parks and

   subdivisions shall be consistent with Article 1, Sections B, C, and D of this ordinance.

(2) All proposals for the development of subdivisions including the placement of

  manufactured home parks and subdivisions shall meet Development Permit requirements of

 Article 3, Section C; Article 4, Section C; and the provisions of Article 5 of this ordinance.

(3) All subdivision proposals including the placement of manufactured home parks and

  subdivisions shall have adequate drainage provided to reduce exposure to flood hazards.

(4) All subdivision proposals including the placement of manufactured home parks and

      subdivisions shall have public utilities and facilities such as sewer, gas, electrical and water

   systems located and constructed to minimize or eliminate flood damage.

CERTIFICATION

It is hereby found and declared by Elk Ridge City:
that severe flooding has occurred in the past within its jurisdiction and will certainly occur within

the future; that flooding is likely to result in infliction of serious personal injury or death, and is

likely to result in substantial injury or destruction of property within its jurisdiction; in order to

effectively comply with minimum standards for coverage under the National Flood Insurance

Program; and in order to effectively remedy the situation described herein, it is necessary that this

ordinance become effective immediately.

Therefore, an emergency is hereby declared to exist, and this ordinance, being necessary for the

immediate preservation of the public peace, health and safety, shall be in full force and effect

from and after its passage and approval.

APPROVED: _________________________________________

(community official)

PASSED: _________________________

(date)

I, the undersigned,__________________________________ , do hereby certify that the above is a

true and correct copy of an ordinance duly adopted by the____________________________ , at a

regular meeting duly convened on ______________________ .

___________________________

      (Secretary or responsible person)

(SEAL)

PENALTIES FOR NONCOMPLIANCE

No structure or land shall hereafter be constructed, located, extended, converted, or

altered without full compliance with the terms of this ordinance and other applicable

regulations. Violation of the provisions of this ordinance by failure to comply with any of

its requirements (including violations of conditions and safeguards established in

connection with conditions) shall constitute a misdemeanor. Any person who violates

this ordinance or fails to comply with any of its requirements shall upon conviction

thereof be fined not more than $750.00 or imprisoned for not more than 90 days,

or both, for each violation, and in addition shall pay all costs and expenses involved in the

case. Nothing herein contained shall prevent the Elk Ridge City 

from taking such other lawful action as is necessary to prevent or remedy any violation.
