MILFORD CITY
REQUEST FOR PROPOSAL
DESIGN-BUILD ROAD CONSTRUCTION
Deadline for all Proposals is Thursday May 21, 2020
Introduction

It is the intent of Milford City to solicit competitive sealed proposals from qualified contractors with the ability and capacity to design, construct, manage, and provide all construction administration for the proposed project.
Background and Objective
Milford City would like to reconstruct approximately 255 lineal feet of 400 South between 100 West and Main Street.  They would like to reduce the existing grade to allow for a more gradual transition onto the driveway accesses along this section of road.  Beaver County Fire District #2 will be constructing a new office building at the northwest corner of 400 South and Main Street.  The Fire District Project will extend the curb & gutter and sidewalk approximately 110 feet to the West, along the North side of 400 South.  The proposed 400 South reconstruction project will require an additional 50 feet of curb & gutter and sidewalk.  
Scope of Services
The Scope of work for this project will consist of roadway reconstruction, obtaining required necessary permits from the state and local government agencies, staking any necessary lines and grades, traffic control including permanent construction signing and daily work area signing, asphalt cutting, roadway milling, necessary erosion control, base course, concrete curb & gutter, concrete driveway, concrete sidewalk, and final cleanup.  Exhibit 1 depicts a general idea of the roadway reconstruction.
All the anticipated work will be conducted within the Milford City rights-of-way.

At the direction of the City, the successful contractor will provide specified services to the City for the terms of the respective agreement(s).  The anticipated services shall include, but are not limited to the following:

· The contractor is required to obtain all necessary permits from the state and local government agencies.

· Necessary survey staking to accurately determine the lines and grades of the project.
· Traffic control which shall include all permanent and daily work construction signing.
· Asphalt cutting shall be required at the transitions from existing asphalt to the reconstructed portion of the roadway.

· The roadway shall be rotomilled as necessary to reduce the roadway cross slopes.  Exhibit 1 depicts the anticipated roadway cross slopes.  In general, the roadway cross slopes shall be as close to 2% as possible while leaving a center crown.  When possible, the min. cross slope shall be 1.5% or greater, and not exceed 3.5%.
· The contractor will be required to provide necessary measures for erosion control.
· Subgrade preparation shall be in accordance to the Milford City General Road Construction Standards and Drawings.  The contractor shall provide a compacted base course for the roadway.  At a minimum, 6 inches of untreated base course shall be compacted to 95%.
· Provide a finish course surface in accordance to the Milford City General Road Construction Standards and Drawings. The contractor shall use 3” of approved bituminous base course BSC
· Provide approximately 50 lineal feet of concrete curb & gutter in accordance to the Milford City General Road Construction Standards and Drawings.  The curb & gutter shall tie the existing curb to the proposed curb for the Beaver County Fire District Office that will be constructed this summer.
· Provide a 24 wide concrete driveway approach, and concrete sidewalk as shown in Exhibit 1.

· Milford City Construction Standards can be found at  https://milford.municipalcodeonline.com/book?type=ordinances#name=15.06_Road_And_Street_Construction  
· The selected Bidder will be required to provide the services of an independent, certified materials testing company to provide materials testing for the subgrade, asphalt, and concrete surfaces.

· All bidders should visit the site to observe the existing conditions prior to submitting a proposal.

· It is noted that the manhole and sewer line in 400 S are very shallow. The selected contractor shall take care not to damage or disrupt the existing sewer line.

Proposal Contents:

1. The Bidder’s proposal shall include a project approach describing the work that the bidder proposes to perform. The approach should include a description of the methods proposed to accomplish the work, the materials proposed for use on the project, a traffic control plan, a materials testing plan, and a project management plan including project meetings and communications with the Owner.

2. The Bidder’s cost proposal should be broken down into individual costs in tabular form for each of the following categories for the work described above and represented in the attached exhibit. For each category, provide the estimated quantity of work to be performed, the unit cost, and the total cost for each category. Provide a total project cost at the bottom, which should be a sum of all subcategory costs.

a. Mobilization (lump sum)

b. Rotomill Existing Road Surface (Square Yards)

c. Untreated Base Course (Cubic Yards)

d. Bituminous Surface Course (Square Yards)

e. Curb and Gutter (Linear Feet)

f. Concrete Driveway Approach and Sidewalk (Lump Sum)

3. All project costs should be represented in the unit costs for the subcategories listed above. Separate payment will not be made for auxiliary tasks not listed above.
  Proposal Submittal Instructions
1. All proposals must be delivered to Milford City by 2:00 p.m. on Thursday May 21, 2020.   Six copies of the RFP’s are required.

2. Bids shall be submitted with two bid schedules.
· Bid Schedule ‘A’ will be considered the Base Bid.
· Bid Schedule ‘B’ will be considered an additive alternate to the project.

 Exhibit 1 has a dividing line that represents the division between Schedule ‘A’ & Schedule ‘B’.  If the City elects to include Bid Schedule ‘B’ as part of the project, the City will award the contract to the lowest responsive responsible bidder for Schedule ‘A’ & Schedule ‘B’ combined.  If the City elects NOT to include Bid Schedule ‘B’ as part of the project, the City will award the contract to the lowest responsive responsible bidder for Schedule ‘A’.
3. Submit proposals to:

Milford City

PO Box 69
26 South 100 West

Milford, Utah 84751
Contact Person:


Makayla Bealer, City Administrator
City Office:  435-387-2711

Public Works Contact for Questions:

Benjamin Stewart

435-463-9568

Nolan Davis, Mayor





Phone:  435-691-9111


