
10-6-5: LOCATION REQUIREMENTS:
Front Setback: 
1. Main Setback:  All dwellings and other structures shall be set back according to the special conditions noted below:
a. The legal property line of the residential lot is located at the back of street curb or back of pavement in the case that there is no curb, twenty feet (20’) from the front lot line.
b. The legal property line of the residential lot is located within the street pavement or gravel area,  forty feet (40’) from the front lot line.
c. The legal property line of the residential lot is located more than ten feet (10’) from the street pavement or gravel area, ten feet (10’) from the front lot line.  Where the legal property line of the residential lot line is angular to the roadway and there is less than ten feet (10’) between the legal property line and the street pavement or gravel area, then a minimum of twenty feet (20’) from the nearest point of the street pavement or gravel area.
