CMPO Transportation Corridor Agreement Feb. 2018
Streets in Hyde Park City
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North/South Corridors

Hiway US91/600W – Principal Arterial - UDOT
200E/400W/CMPO – Minor Arterial - 99’ ROW - from 1400N to Smithfield
400E/100W – Minor Collector – 66’ ROW
800E/250E – Minor Collector – 66’ ROW
1200E/700E – Major Collector – 66’ ROW from 1400N to 4400N
·         80’ ROW from 4400N to Smithfield
1600E/1000E – Minor Collector – 66’ ROW
Power Line Corridor – 66’ ROW
200W/800W – Major Collector – 80’ ROW
400W/1000W – Minor Collector - 66’ ROW

East/West Corridors

3100N/600S – Major Collector – 80’ ROW from 400W to US91, and 800E/250E to 1200E/700E
	            Minor Arterial – 80’ ROW from US91 to 800E/250E, Minor Collector 66’ ROW 
            from 1200E/700E to Power Line Corridor
3500N/200S – Major Collector – 80’ ROW from 400W to 200W
				 66’ ROW from 200W to Power Line Corridor
3700N/Center Street – Major Collector – 80’ ROW
4200N/450N – Major Collector – 80’ ROW from US91 to 100W
·          66’ ROW from  100W to 1000E
4400N/650N – Minor Collector – 66’ ROW

Inventory of Existing Built Corridors
North/South  (profiles from west to east)

US91/600W 
@3100N/600S – 99’ROW – 6’walk, 4’park strip, 10’shoulder, 24’travel, 12’turn, 24’travel, 10’shoulder, 9’swale
@3700N/Center Street – 99’ – 10’swale, 10’shoulder, 24’travel, 12’turn, 24’travel, 10’shoulder, 4’park strip, 4’walk
@4200N/450N -  99’ROW – 10’swale, 9’shoulder, 24’travel, 12’turn, 24’travel, 9’shoulder, 10’swale

200E/400W/CMPO    
@1500N – 99’ROW – 5’walk, 8’park strip, 17’shoulder, 33’asphalt, 17’shoulder, 8’park strip, 10’walk
@1800N -  99’ROW – 5’walk, 8’park strip, 7’shoulder, 54’asphalt, 7’shoulder, 8’ park strip, 10’walk
@2000N -  99’ROW – 25’ swale, 7’shoulder, 33’asphalt, 7’shoulder, 16’park strip, 10’walk
@2200N – 99’ROW – 5’walk, 8’park strip, 30’asphalt, 8’median, 21’aspahlt, 16’swale, 10’walk

1200E/700E
@Shadow Bluff – 85’ROW – 8’walk, 14’park strip, 45’aspahlt, 14’park strip, 4’walk
@Krebs/Lions Park trail – 80’ROW – 5’walk, 10’park strip, 18’asphalt, 12’median, 18’asphalt, 10’ park strip, 5’walk
@Foothill Heights – 80’ROW – 5’walk, 5’park strip, 29’asphalt (half the street)
@300N/Greystone – 80’ROW – 25’swale, 30’asphalt, 25’swale
@450N/Mt.Gate – 80’ROW – 4’walk, 8’park strip, 54’asphalt, 8’park strip, 4’walk

East/West  (profiles  from north to south)

3100N/600S
400W/1000W to US91 – 80’ROW – 7’edge, 4’walk, 6’park strip, 45’asphalt, 18’swale
US91/600W to 150W – 80’ROW
150W to 100W – 80’ROW – 4’walk, 8’park strip, 54’asphalt, 8’park strip, 4’walk
100W to 50E – 66’ – temp road
50E to 250E – 22’ – farm road
250E to Park Meadow Drive – 60’ – (half road) 23’asphalt, 3’park strip, 4’walk
Park Meadow Drive to 475E – 80’ROW – 4’walk, 8’park strip, 54’asphalt, 8’park strip, 4’walk

3500N/200S  
200W to 100W – 99’ROW – 4’walk, 32’swale, 25’asphalt, 32’swale, 4’walk
100W to Main – 99’ROW – 4’walk, 32’swale, 40’asphalt, 6’park strip, 5’walk, 10’edge
Main to 50E – 99’ROW
50E to 100E – 89’
100E to 200E – 80’
200E to 250E – 70’
250E to 400E – 70’ / 45’
@bridge – 40’ - 5’walk, 22’asphalt
400E to Church – 40’
Church to 700E – 42’
700E to 800E – 60’ROW
800E to 1000E – 66’ROW

3700N/Center Street
350W/950W to 200W/800W – 99’ ROW – 6’walk, 7’park strip, 50’asphalt, 30’plant strip, 4’walk 
200W/800W to US91/600W – 66’ ROW – 4’walk, 40’asphalt, 21’swale
US91/600W to 200W – 80’ – 6’walk, 27’swale, 26’asphalt, 20’swale
200W to 100E – 99’ROW – 5’walk, 18’swale, 40’asphalt, 35’swale
100E to 200E – 99’ROW – 4’walk, 28’swale, 30’asphalt, 36’swale
200E to 400E – 66’ROW – 27’swale, 24’asphalt, 15’swale
400E to 500E – 60’ROW – 13’swale, 24’asphalt, 23’swale
500E to Lions Park – 45’ROW – 13’swale, 5’walk, 27’asphalt
Lions Park to 700E – 30’asphalt

4200N/450N
300W to 200W – 66’ROW – (half street) 22’asphalt, 6’park strip, 4’walk
200W to 100W – 66’ROW – 4’walk, 3’plant strip, 50’asphalt, 3’plant strip, 4’walk
100W to 100E – 66’ROW – temp road
100E to 300W – 66’ROW – (half street) 22’asphalt, 6’park strip, 4’walk
300E to 400E – 66’ROW – 4’walk, 3’plant strip, 50’asphalt, 3’plant strip, 4’walk
400E to 475E – 66’ROW – (3/4 street) 38’asphalt, 8’swale, 4’walk
475E to 600E – 66’ROW – (5/8 street) 30’asphalt, 8’swale, 4’walk
600E to 800E – 66’ROW – 4’walk, 8’park strip, 40’asphalt, 8’park strip, 4’walk


