Glendale Town

2020 Annual Drinking Water Quality

     We are, including cross connect pleased to provide you with this year's Annual Water Quality Report. We want to keep you informed about the excellent water and services we have delivered to you over the past year. Our goal is and always has been, to provide to you a safe and dependable supply of drinking water. Our water sources are Lydia’s Canyon Spring, and Hop’s Well.

     The Drinking Water Source Protection Plan for Glendale Town is available for your review.  It contains information about source protection zones, potential contamination sources and management strategies, including cross connection control program to protect our drinking water.  Potential contamination sources common in our protection areas are roads, .  Our sources have a low- level susceptibility to potential contamination.  We have also developed management strategies to further protect our sources from contamination.  Please contact us if you have questions or concerns about our source protection plan.   

     This report shows our water quality and what it means to our customers. 

     If you have any questions about this report or concerning your water utility, please contact Ellen Lamb – (435) 648-2341. We want our valued customers to be informed about their water utility. If you want to learn more, please attend any of our regularly scheduled meetings. They are held on the 3rd Thursday of each month at 7:00pm at town hall.

     Glendale Town routinely monitors for constituents in our drinking water in accordance with the Federal and Utah State laws. The following table shows the results of our monitoring for the period of January 1st to December 31st, 2020. All drinking water, including bottled drinking water, may be reasonably expected to contain at least small amounts of some constituents.  It is important to remember that the presence of these constituents does not necessarily pose a health risk. 

     In the following table you will find many terms and abbreviations you might not be familiar with. To help you better understand these terms we have provided the following definitions:

Non-Detects (ND) - laboratory analysis indicates that the constituent is not present.

ND/Low - High - For water systems that have multiple sources of water, the Utah Division of Drinking Water has given water systems the option of listing the test results of the constituents in one table, instead of multiple tables. To accomplish this, the lowest and highest values detected in the multiple sources are recorded in the same space in the report table. 

 Parts per million (ppm) or Milligrams per liter (mg/l) - one part per million corresponds to one minute in two years or a single penny in $10,000.

Parts per billion (ppb) or Micrograms per liter (ug/l) - one part per billion corresponds to one minute in 2,000 years, or a single penny in $10,000,000. 

Parts per trillion (ppt) or Nanograms per liter (nanograms/l) - one part per trillion corresponds to one minute in 2,000,000 years, or a single penny in $10,000,000,000.

Picocuries per liter (pCi/L) - picocuries per liter is a measure of the radioactivity in water.

Nephelometric Turbidity Unit (NTU) - nephelometric turbidity unit is a measure of the clarity of water. Turbidity in excess of 5 NTU is just noticeable to the average person.

Action Level (AL) - the concentration of a contaminant which, if exceeded, triggers treatment or other requirements which a water system must follow.

Date- Because of required sampling time frames i.e. yearly, 3 years, 4 years and 6 years, sampling dates “May” seem out of date.

Waivers (W)- Because some chemicals are not used or stored in areas around drinking water sources, some water systems have been given waivers that exempt them from having to take certain chemical samples, these waivers are also tied to Drinking Water Source Protection Plans. 

	TEST RESULTS

	Contaminant
	Violation

Y/N
	Level 

Detected

ND/Low-High
	Unit

Measurement
	MCLG
	MCL
	Date Sampled
	Likely Source of Contamination

	Microbiological Contaminants

	Total Coliform Bacteria                                    
	y

	1
	N/A
	0
	Presence of coliform bacteria in 5% of monthly samples
	2016
	Naturally present in the environment

	. Fecal coliform and             E.coli
	N
	0
	N/A
	0
	a routine sample and repeat sample are total coliform positive, and one is also fecal coliform or E. coli positive
	2016
	Human and animal fecal waste

	Turbidity 

for Ground Water
	N
	.82
	NTU

 TC "NTU" \l 5 

	N/A

 TC "N/A" \l 5 

	5
	2019
	Soil runoff

	Radioactive Contaminants

	 Alpha emitters    
	N
	1.6
	pCi/1
	0
	15
	2019
	Erosion of natural deposits

	Radium 228
	N
	1.3
	pCi/1
	0
	5
	2019
	Erosion of natural deposits

	Inorganic Contaminants

	 Arsenic
	N
	1.4
	Ppb
	0
	.001
	2019
	Erosion of natural deposits; runoff from orchards; runoff from glass and electronics production wastes

	 Barium
	N
	0.198
	ppm
	2
	2
	2019
	Discharge of drilling wastes; discharge from metal refineries; erosion of natural deposits

	 Copper 

90% results

a. # of sites that exceed the AL
	N


	A.0.026
b.0
	ppm
	1.3
	AL=1.3
	2019
	Corrosion of household plumbing systems; erosion of natural deposits

	Fluoride
	N
	0.7
	ppm
	4
	4
	2019
	Erosion of natural deposits; water additive which promotes strong teeth; discharge from fertilizer and aluminum factories

	Lead

b.   90% Results

c. # of sites that exceed the

AL
	N
	a. 00.15
b. 0
	ppb
	0
	AL=15
	2019
	Corrosion of household plumbing systems, erosion of natural deposits

	Nitrate (as Nitrogen)
	N
	ND
	PPM
	10
	10
	2021
	Runoff from fertilizer use; leaching from septic tanks, sewage; erosion of natural deposits

	Sodium
	N
	2
	ppm
	None set by EPA
	None set by EPA
	2019
	Erosion of natural deposits; discharge from refineries and factories; runoff from landfills.

	Sulfate
	N
	9
	ppm
	500*
	1000
	2019
	Erosion of natural deposits; discharge from refineries and factories; runoff from landfills, runoff from cropland

	TDS (Total Dissolved Solids
	N
	202
	ppm
	2000**
	1000**
	2019
	Erosion of natural deposits

	


     All sources of drinking water are subject to potential contamination by constituents that are occurring or are man-made.  Those constituents can be microbes, organic or inorganic chemicals, or radioactive materials.  All drinking water, including bottled water, may reasonably be expected to contain at least small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that the water poses a health risk. More information about contaminants and potential health effects can be obtained by calling the Environmental Protection Agency’s Safe Drinking Water Hotline at 1-800-426-4791.

     MCL’s are set at very stringent levels. To understand the possible health effects described for many regulated constituents, a person would have to drink 2 liters of water every day at the MCL level for a lifetime to have a one-in-a-million chance of having the described health effect.

     Water samples taken in March 2019 confirmed the presence of total coliform bacteria.  Total coliforms are common in the environment and are generally not harmful themselves.  The presence of these bacteria is usually a result of a problem with water treatment or the pipes which distribute the water and indicates that the water may have been contaminated with organisms that can cause disease.  Symptoms may include diarrhea, cramps, nausea, and possible jaundice, and any associated headaches and fatigue.  When the monthly samples confirmed the presence of total coliform bacteria we took steps to identify and correct the problem.  Subsequent monthly sampling has confirmed the absence of total coliforms in the water system.

     Cross Connection Customer Education:

There are many connections to our water distribution system.  When connections are properly installed and maintained, the concerns are very minimal.  However, unapproved and improper piping changes or connections can adversely affect not only the availability, but also the quality, of the water.  A cross connection may let polluted water or even chemicals mingle into the water supply system when not properly protected.  This not only compromises the water quality but can also affect your health.  So, what can we do?  Do not make or allow improper connections at your homes.  Even that unprotected garden hose lying in the puddle next to the driveway is a cross connection.  The unprotected lawn sprinkler system after you have fertilized or sprayed is also a cross connection.  When a cross connection is allowed to exist at your home it will affect you and your family first.  If you would like to learn more about helping to protect the quality of our water, call us for further information about ways you can help. We worked with State officials and specific homeowners to remove potential cross connection hazards in homes with after- market booster pumps This was a taxing and confusing issue for the homeowners but all the parties involved worked hard and diligently to meet specifications allowing modification to the specific homes. The state and Glendale Town will no longer allow even modified booster pumps on the Glendale Culinary system
     If present, elevated levels of lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. Glendale Town is responsible for providing high quality drinking water, however, we cannot control the variety of materials used in plumbing that all our customers help us protect our water sources, which are the heart of our community, our way of life and our children’s future.  If you have any questions regarding cross connection hazard or other water issues, please feel free to contact John Phillips, Glendale Certified Water Operator at:  435 648 2341. Thank you.

A copy of this report is available at the Glendale Town office

components. When your water has been sitting for several hours, you can minimize the potential for lead exposure by flushing your tap for 30 seconds to 2 minutes before using water for drinking or cooking. If you are concerned about lead in your water, you may wish to have your water tested. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available from the safe Drinking Water Hotline or at http://www.epa.gov/safewater/lead.

     Some people may be more vulnerable to contaminants in drinking water than the                       general population. Immuno-compromised persons such as persons with cancer                        undergoing chemotherapy, persons who have undergone organ transplants, people with                 HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections. These people should seek advice about drinking water from their health care providers. EPA/CDC guidelines 

on appropriate means to lessen the risk of infection by cryptosporidium and other microbiological contaminants are available from the Safe Drinking       Water Hotline (800-426-4791).  

     We at Glendale Town work around the clock to provide top quality water to every tap.  ask 

We 

Brandi Smith
CCR Compliance

Division of Drinking Water

P.O. Box 144830

Salt Lake City, Utah 84114-4830

Dear Ms. Smith
Subject:   Consumer Confidence Report for Glendale Town # 13004
                  Enclosed is a copy of Glendale Town Consumer Confidence Report.  It contains water   

                 quality information for our water system for the calendar year 2020 or the most recent sample    

                 data.

We have delivered this report to our customers by:
Posting on Public Notice Website and Glendale Social Media and posting at the Glendale Town 
Posting a notice of the availability of the report on our water bill and then sending a copy to those that request it.  We also allow inspection of the report at the water system office.

If you have any questions, please contact me at Glendale Town 435-648-2341
Sincerely,
John Phillips
Glendale Town Water
UTAH13004


