
SIGURD TOWN
P.O. BOX 570064 SIGURD, UTAH 84657 ∙ 435-896-4645

An Invitation to Bid 
Competitive Sealed Proposals (CSP) for a procurement of upgrades and improvements to the Sigurd Town Cemeteries.

Document Summary
Sigurd Town is seeking Competitive Sealed Proposals (CSP) for procurement of upgrades and improvements to Sigurd Town Cemetery and Vermillion Cemetery. The project is funded through a Community Development Block Grant (CDBG). Sigurd Town will select (1) engineering firm and (1) subcontractor to provide equipment, materials, surveying and architectural work and labor as outlined in this request.

Scope of Work
To make improvements to the two existing cemeteries in Sigurd Town. 
The first cemetery being Sigurd Town Cemetery at 780 West Substation Road in Sigurd will have a 7200 sq ft parking surface upgraded with asphalt or similar surfacing. 
The existing driveways will have potholes filled in and the surfacing will be replaced with asphalt or similar surfacing to prevent road wear and discourage weed growth. An additional drive lane will be added to utilize an unused portion of the property owned by Sigurd Town and make space available for expansion of the cemetery. The drive lanes will be approximately 12 ft wide and total approximately 1640 linear ft. 
The dilapidated livestock mesh fencing will be replaced with a decorative fencing more fitting for the property needs. The fencing requirement totals approximately 1560 linear ft.  
The other cemetery owned by Sigurd Town is the Vermillion Cemetery located at 1530 N South Canyon Road.
This cemetery requires approximately 30,000 sq ft of adequate surfacing for its parking area to prevent wear and discourage weed growth.
The 12 ft wide drive lane is approximately 350 linear ft to be resurfaced with asphalt or appropriate surfacing to prevent wear and discourage weed growth.
The damaged and unsightly chain link fence is to be replaced with approximately 1400 square ft of decorative fencing fitting to the property needs.
The CSP shall include all costs associated with proposed cemetery improvements and upgrades.

Questions Regarding the CSP should be directed to:
Sigurd Town
(435)896-4645
sigurdtown@cut.net
	or
Attn: Joe Kirkwood 
(435)287-8508
joekirkwood.jk@gmail.com

Design Guidelines 
Suppliers should base their designs with functionality and longevity in mind. Accessibility and safety standards, quality of components, quality of design, value to the end user, handicapped accessibility, inclusiveness, cost, appropriateness to location and target demographic must be considered in the design of the cemetery improvements. (Contact the above listed number for further demographic information).

The total dollar amount allocated to complete the full project has a target amount of $255,326.00. Please provide proposals that fit withing this budget amount. Any proposal exceeding $00.00 beyond the budgeted amount will be automatically denied.

Required Items:

1. Parking area with asphalt or other adequate surfacing as allowed by budget.
2. Redevelopment or paving of existing driveways to provide maximum longevity as allowed by budget.
3. Fencing must be appropriate to the demographic and be both aesthetically pleasing and structurally robust with the ability to repair in mind. Fencing proposal will include removal of existing fencing.
4. Development/ engineering of approximately 450 linear feet of new driveway. 
5. All asphalt/ surfacing will be designed to discourage weed growth maintain cemetery appearance.

Assembly/Installation, Inspection and Warrantee
Assembly/Installation: The cemetery improvements and installation will be provided by and managed by the Supplier or engineering firm. The Supplier will provide direct supervision or provide qualified and certified representation familiar with the project parameters. All equipment, tools and machinery required for the project will be provided by the Supplier will be given 365 calendar days to complete proposed work included demolition, surveying, design, manufacturing, delivery, and installation. Calendar days will begin as outlined in the awarded bid/contract. 
Inspection: A certified representative of the Supplier is required to conduct a post installation inspection of all cemetery improvements and upgrades upon completion to insure proper installation. If not properly installed, modifications must be discussed with the Town and remedied immediately. Co-inspection with the Supplier’s representative will be conducted with Sigurd Town personnel following installation. The supplier will submit to Sigurd Town a Certificate of Completion and Warrantee upon approval of co-inspection. 
Warrantee: Upon completion of installation, the Supplier will provide documentation attesting that the project has been competently completed and will be free from defects in material or workmanship. 

Compliance
All equipment must meet or exceed federal guidelines. Documentation of compliance must be provided with the document’s proposal.
All designs must comply with the Americans with Disabilities ACT (ADA). 
The selected supplier with be required to comply with the requirements of the CDBG funding source. These requirements will be made part of the installation contract that will be entered into following supplier selection. The CDBG requirements include compliance with 4010 Federal Labor Standards, the CDBG Supplemental Conditions and David-Bacon Building wage Rates.
The Supplier will ensure that hiring is made on the basis of merit and qualifications and that there will be no discrimination in employment on the basis of race, ancestry, color, physical or mental disability, religion, national origin, sex, age, marital or familial status, creed, ex-offender status, physical condition, political belief, public assistance status, or sexual orientation, gender identity, except where these criteria are reasonable bona fide occupational qualifications.
The Supplier will utilize the Utah Davis-Bacon Wage Rates for Heavy Construction effective to the most recent date posted prior to bidding.
The Supplier must provide an original Certificate of Product Liability Insurance. 

Disclaimer
Sigurd Town will be exempt from any liability for costs incurred by unsuccessful suppliers in the preparation of a CSP.

Proposal Submittal Date and Time
All CSP must be submitted to Sigurd Town by 4pm 12/07/2022.
Sigurd Town office 595 North State Street Sigurd Utah, (435)896-4645.
All submitted CSP will be addressed as follows:
Proposal for Sigurd Town Cemeteries Improvements

Proposal Format
Proposals shall be submitted in the following format:
● Project Name
● Supplier Name
● Statement that CSP meets CDBG Guidelines
● The project's proposed description, photos, plans, etc.
● Designs showing all safety precautions necessary for this park project
● Warrantee and insurance capabilities
● Statement of understanding of Davis-Bacon and non-discrimination requirement
● Project Cost Proposal & Timeline
● Any additional information relating to scoring criteria as listed below
● References

Civil Rights Statement
Qualified women, veterans, minority, and handicapped individuals are strongly encouraged to submit proposals.

Evaluation and Selection Process
Proposals will be evaluated by the Sigurd Town Council based on the following criteria:

Criteria & Points:
1. CSP Proposed Cost & Timeline (20 Points)
2. CSP addresses design guidelines and specifications (20 Points)
3. CSP Statement to meet CDBG guidelines (20 Points)
4. CSP Safety precautions, warrantee, and insurance capabilities (20 Points)
5. Overall Quality of CSP and references (20 Points)
Maximum Points: 100






	
	*Sigurd Town is an equal opportunity provider*	
